{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":48,"n_cols":11,"rows_kept":48,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","2AMXM-M"]
[]
[]
[]
[]
["","","","","","2AMXM40M3V1B","2AMXM40M4V1B","2AMXM50M2V1B","2AMXM50M4V1B","2AMXM50M3V1B","2AMXM40M2V1B (Archived)"]
["Ventilator-","Luchthoeveelheid","Koelen","Superlaag","m³/min","","","34","","","30"]
["","","Verwarmen","Superlaag","m³/min","","","34","","","32"]
["Geluidsvermogenniveau","Verwarmen","","","dB(A)","","62","","62"]
["","Koelen","","","dB(A)","","60","","60"]
["Ventilator-","Luchthoeveelheid","Koelen","Superlaag","cfm","","","1200","","","1059"]
["","","Verwarmen","Superlaag","cfm","","","1200","","","1130"]
["Afmetingen","Unit","","Hoogte","mm","550","550","550","550","550","550"]
["","","","Breedte","mm","765","765","765","765","765","765"]
["","","","Diepte","mm","285","285","285","285","285","285"]
["Gewicht","Unit","","","kg","36","36","41","41","41","36"]
["Ventilatormotor","Snelheid","Koelen","Superlaag","rpm","500","500","890","500","500","760"]
["","","Verwarmen","Superlaag","rpm","320","320","890","500","500","820"]
["Compressor","Type","","","","Hermetisch gesloten swingcompressor","Hermetisch gesloten swingcompressor","Hermetisch gesloten swingcompressor","Hermetisch gesloten swingcompressor","Hermetisch gesloten swingcompressor","Hermetisch gesloten swingcompressor"]
["Werkingsbereik","Koelen","","Min.","°C DB","","46.0","-10","46.0","","-10"]
["","","","Max.","°C DB","","-10","46","-10","","46"]
["","Verwarmen","","Min.","°CWB","","-15","-15","-15.0","","-15"]
["","","","Max.","°CWB","","18.0","18","18.0","","18"]
["Geluidsdrukniveau op 1 m","Koelen","","Geluidsdrukniveau op 1 m-=-Koelen-=-Hoog-=-dB(A)","dB(A)","46","46","","48","48"]
["","","","Nom.","dB(A)","","","46","","","48"]
["","Verwarmen","","Geluidsdrukniveau op 1 m-=-Verwarmen-=-Hoog-=-dB(A)","dB(A)","48","48","","50","50"]
["","","","Nom.","dB(A)","","","48","","","50"]
["Koelmiddel","Type","","","","R-32","R-32","R-32","R-32","R-32","R-32"]
["","Vulling","","","kg","0.88","0.88","1.15","1.15","1.15","0.88"]
["Koudemiddel","Vulling","","","tCO2Eq","0.59","0.6","0.8","0.78","0.78","0.6"]
["Koelmiddel","GWP","","","","675.0","675","675","675","675","675"]
["Koelleidingmaten","Leidinglengte","","Max.","m","20","20 (1)","20","20 (1)","20","20"]
["Leidingaansluitingen","Bijkomende koelmiddelvulling","","","kg/m","0,02 (voor leidinglengte van meer dan 20 m)","0,02 (voor leidinglengte van meer dan 20 m)","0,02 (voor leidinglengte van meer dan 20 m)","0,02 (voor leidinglengte van meer dan 20 m)","0,02 (voor leidinglengte van meer dan 20 m)","002 (voor leidinglengte van meer dan 20 m)"]
["Koelleidingmaten","Hoogteverschil","","Max.","m","15.0","15","15","15","15.0","15"]
["","","IU - IU","Max.","m","7.5","7.5","7.5","7.5","7.5","7.5"]
["","Totale leidinglengte","Systeem","Werkelijk","m","30","30","30","30","30","30"]
["Standaard-accessoires","Installation manual","","","","1","1","1","1","1","Installation manual"]
["","Drain plug","","","","1","1","1","1","1","Drain plug"]
["","Screw bag","","","","1","1","1","1","1","Screw bag"]
["Voeding","Fase","","","","1~","1~","1~","1~","1~","1~"]
["Spanningsvorm","Frequentie","","","Hz","50","50","50","50","50","50"]
["","Spanning","","","V","220-230-240","220-230-240","220-240","220-230-240","220-230-240","220-240"]
["Opmerkingen","","","","","(1) - Van één kamer","","","","(1) - Van één kamer","(1) - Bevat gefluoreerde broeikasgassen"]
["","","","","","","(1) - Van één kamer","","(1) - Van één kamer"]
["","","","","","","(2) - See separate drawing for operation range","","(2) - See separate drawing for operation range"]
["","","","","","","(3) - See separate drawing for electrical data","","(3) - See separate drawing for electrical data"]
["","","","","","","(4) - Bevat gefluoreerde broeikasgassen","","(4) - Bevat gefluoreerde broeikasgassen"]
["Standaard-accessoires","Reducer assembly","","","","","","1","1","1"]