{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":39,"n_cols":7,"rows_kept":39,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","2MXF-A"]
[]
[]
[]
[]
["","","","","","2MXF40A2V1B (Archived)","2MXF50A2V1B (Archived)"]
["Afmetingen","Unit","","Hoogte","mm","550","550"]
["","","","Breedte","mm","765","765"]
["","","","Diepte","mm","285","285"]
["Gewicht","Unit","","","kg","36","41"]
["Ventilatormotor","Snelheid","Koelen","Superlaag","rpm","500","500"]
["","","Verwarmen","Superlaag","rpm","320","500"]
["Compressor","Type","","","","Hermetisch gesloten swingcompressor","Hermetisch gesloten swingcompressor"]
["Werkingsbereik","Koelen","","Min.","°C DB","-10","-10"]
["","","","Max.","°C DB","46","46"]
["","Verwarmen","","Min.","°CWB","-15","-15"]
["","","","Max.","°CWB","18","18"]
["Geluidsdrukniveau op 1 m","Koelen","","Hoog","dB(A)","46","48"]
["","Verwarmen","","Hoog","dB(A)","48","50"]
["Koelmiddel","Type","","","","R-32","R-32"]
["","Vulling","","","kg","0.88","1.15"]
["Koudemiddel","Vulling","","","tCO2Eq","0.60","0.78"]
["Koelmiddel","GWP","","","","675","675"]
["Koelleidingmaten","Leidinglengte","","Max.","m","20 (1)","20 (1)"]
["Leidingaansluitingen","Bijkomende koelmiddelvulling","","","kg/m","002 (voor leidinglengte van meer dan 20 m)","002 (voor leidinglengte van meer dan 20 m)"]
["Koelleidingmaten","Hoogteverschil","","Max.","m","15.0","15.0"]
["","","IU - IU","Max.","m","7.5","7.5"]
["","Totale leidinglengte","Systeem","Werkelijk","m","30","30"]
["Standaard-accessoires","Installation manual","","","","1","1"]
["","Drain plug","","","","1","1"]
["","Screw bag","","","","1","1"]
["Voeding","Fase","","","","1~","1~"]
["Spanningsvorm","Frequentie","","","Hz","50","50"]
["","Spanning","","","V","220-230-240","220-230-240"]
["Opmerkingen","","","","","(1) - Van één kamer","(1) - Van één kamer"]
["","","","","","(2) - Zie afzonderlijke afbeelding voor bedrijfsbereik","(2) - Zie afzonderlijke afbeelding voor bedrijfsbereik"]
["","","","","","(3) - Voor elektrische gegevens zie afzonderlijke tekening","(3) - Voor elektrische gegevens zie afzonderlijke tekening"]
["","","","","","(4) - Bevat gefluoreerde broeikasgassen","(4) - Bevat gefluoreerde broeikasgassen"]
["Standaard-accessoires","Reducer assembly","","","","","1"]