{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":8,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","2MXM-N"]
[]
[]
[]
[]
["","","","","","2MXM40N2V1B","2MXM50N2V1B","2MXM68N2V1B"]
["Afmetingen","Unit","","Hoogte","mm","550","550","734"]
["","","","Breedte","mm","765","765","958"]
["","","","Diepte","mm","285","285","340"]
["Gewicht","Unit","","","kg","36","41","60"]
["Ventilatormotor","Snelheid","Koelen","Superlaag","tpm","500","500","420"]
["","","Verwarmen","Superlaag","tpm","320","500","420"]
["Compressor","Type","","","","Hermetisch gesloten swingcompressor","Hermetisch gesloten swingcompressor","Hermetisch gesloten swingcompressor"]
["Werkingsbereik","Koelen","","Min.","°CDB","","","-10"]
["","","","Max.","°CDB","","","46"]
["Geluidsdrukniveau op 1 m","Koelen","","Geluidsdrukniveau op 1 m-=-Koelen-=-Hoog-=-dB(A)","dB(A)","46","48"]
["","","","Nom.","dB(A)","","","48"]
["","Verwarmen","","Geluidsdrukniveau op 1 m-=-Verwarmen-=-Hoog-=-dB(A)","dB(A)","48","50"]
["","","","Nom.","dB(A)","","","48.0"]
["Koelmiddel","Type","","","","R-32","R-32","R-32"]
["","Vulling","","","kg","0.88","1.15","2"]
["Koudemiddel","Vulling","","","tCO2Eq","0.60","0.78","1.35"]
["Koelmiddel","GWP","","","","675","675","675.0"]
["Koelleidingmaten","Leidinglengte","","Max.","m","20","20","25"]
["Leidingaansluitingen","Bijkomende koelmiddelvulling","","","kg/m","0,02 (voor leidinglengte van meer dan 20 m)","0,02 (voor leidinglengte van meer dan 20 m)","0,02 (voor leidinglengte van meer dan 30 m)"]
["Koelleidingmaten","Hoogteverschil","","Max.","m","15.0","15.0","15.0"]
["","","IU - IU","Max.","m","7.5","7.5","7.5"]
["","Totale leidinglengte","Systeem","Werkelijk","m","30","30","50"]
["Standaard-accessoires","Installation manual","","","","1","1","1"]
["","Drain plug","","","","1","1","1"]
["","Screw bag","","","","1","1","1"]
["Voeding","Fase","","","","1~","1~","1~"]
["Spanningsvorm","Frequentie","","","Hz","50","50","50"]
["","Spanning","","","V","220-230-240","220-230-240","220-240"]
["Opmerkingen","","","","","(1) - Van één kamer","(1) - Van één kamer","(1) - Van één kamer"]
["Standaard-accessoires","Reducer assembly","","","","","1","1"]
["","Drain cap","","","","","","3"]