{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":56,"n_cols":11,"rows_kept":56,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","2MXS-H"]
[]
[]
[]
[]
["","","","","","2MXS40H3V1B","2MXS40H3V1B2","2MXS40H2V1B","2MXS50H3V1B","2MXS50H3V1B2","2MXS50H2V1B"]
["Geluidsdrukniveau op 1 m","Verwarmen","","Nom.","dB(A)","48","48","","50","50"]
["","Koelen","","Nom.","dB(A)","47","47","","48","48"]
["Standaard-accessoires","Montagehandleiding","","","","1","1","","1","1"]
["","Zakje schroeven","","","","1","1","","1","1"]
["","Aftapplug","","","","1","1","","1","1"]
["Koelmiddel","Charge","","","TCO2Eq","2.5","2.5","","3.3","3.3"]
["","GWP","","","","2,087.5","2,087.5","","2,087.5","2,087.5"]
["","Vulling","","","kg","1.20","1.20","","1.60","1.60"]
["","Type","","","","R-410A","R-410A","","R-410A","R-410A"]
["Leidingaansluitingen","Hoogteverschil","IU - IU","Max.","m","7.5","7.5","","7.5","7.5"]
["","","","Max.","m","15","15","","15","15"]
["","Bijkomende koelmiddelvulling","","","kg/m","0,02 (voor leidinglengte van meer dan 20 m)","0,02 (voor leidinglengte van meer dan 20 m)","","0,02 (voor leidinglengte van meer dan 20 m)","0,02 (voor leidinglengte van meer dan 20 m)"]
["","Totale leidinglengte","Systeem","Werkelijk","m","30","30","","30","30"]
["Compressor","Type","","","","Hermetisch gesloten swingcompressor","Hermetisch gesloten swingcompressor","","Hermetisch gesloten swingcompressor","Hermetisch gesloten swingcompressor"]
["Afmetingen","Unit","","Breedte","mm","765","765","","765","765"]
["","","","Diepte","mm","285","285","","285","285"]
["","","","Hoogte","mm","550","550","","550","550"]
["Gewicht","Unit","","","kg","38","38","","42","42"]
["Power supply","Fase","","","","1~","1~","","1~","1~"]
["","Frequentie","","","Hz","50","50","","50","50"]
["","Spanning","","","V","220-240","220-240","","220-240","220-240"]
["Opmerkingen","","","","","(1) - Bevat gefluoreerde broeikasgassen","(1) - Bevat gefluoreerde broeikasgassen","","(1) - Bevat gefluoreerde broeikasgassen","(1) - Bevat gefluoreerde broeikasgassen"]
["Afmetingen","Unit","","Hoogte","mm","","","550","","","550"]
["","","","Breedte","mm","","","765","","","765"]
["","","","Diepte","mm","","","285","","","285"]
["Gewicht","Unit","","","kg","","","38","","","42"]
["Compressor","Type","","","","","","Hermetisch gesloten swingcompressor","","","Hermetisch gesloten swingcompressor"]
["Werkingsbereik","Koelen","","Min.","°CDB","","","10","","","10"]
["","","","Max.","°CDB","","","46","","","46"]
["","Verwarmen","","Min.","°CWB","","","-15","","","-15"]
["","","","Max.","°CWB","","","15.5","","","15.5"]
["Geluidsdrukniveau op 1 m","Koelen","","Nom.","dB(A)","","","47","","","48"]
["","Verwarmen","","Nom.","dB(A)","","","48","","","50"]
["Koelmiddel","Type","","","","","","R-410A","","","R-410A"]
["","Vulling","","","kg","","","1.20","","","1.60"]
["Koudemiddel","Vulling","","","tCO2Eq","","","2.5","","","3.3"]
["Koelmiddel","GWP","","","","","","2087.5","","","2087.5"]
["Koelleidingmaten","Leidinglengte","","Max.","m","","","20","","","20"]
["Leidingaansluitingen","Bijkomende koelmiddelvulling","","","kg/m","","","0,02 (voor leidinglengte van meer dan 20 m)","","","0,02 (voor leidinglengte van meer dan 20 m)"]
["Koelleidingmaten","Hoogteverschil","","Max.","m","","","15","","","15"]
["","","IU - IU","Max.","m","","","7.5","","","7.5"]
["","Totale leidinglengte","Systeem","Werkelijk","m","","","30","","","30"]
["Standaard-accessoires","Installation manual","","","","","","1","","","1"]
["","Drain plug","","","","","","1","","","1"]
["","Screw bag","","","","","","1","","","1"]
["Voeding","Fase","","","","","","1~","","","1~"]
["Spanningsvorm","Frequentie","","","Hz","","","50","","","50"]
["","Spanning","","","V","","","220-240","","","220-240"]
["Standaard-accessoires","Montage verloopstuk","","","","","","","1","1"]
["","Reducer assembly","","","","","","","","","1"]