{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":68,"n_cols":7,"rows_kept":68,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","3AMXM-M"]
[]
[]
[]
[]
["","","","","","3AMXM52M3V1B","3AMXM52M2V1B"]
["Geluidsdrukniveau op 1 m","Verwarmen","","Nom.","dB(A)","47"]
["","Koelen","","Nom.","dB(A)","46"]
["Standaard-accessoires","Montagehandleiding","","","","1"]
["","Zakje schroeven","","","","1"]
["","Aftapplug","","","","1"]
["","Afvoerdop (1)","","","","6"]
["","Afvoerdop (2)","","","","3"]
["","Stickervel met F-gaslabel","","","","1"]
["","Label bijkomend koelmiddel","","","","1"]
["Koelmiddel","Charge","","","TCO2Eq","1.2"]
["","GWP","","","","675"]
["","Charge","","","kg","1.8"]
["","Type","","","","R-32"]
["Ventilatormotor","Snelheid","Koelen","Superlaag","rpm","420"]
["","","Verwarmen","Superlaag","rpm","420"]
["Koelleidingmaten","Hoogteverschil","IU - IU","Max.","m","7.5"]
["","","","Max.","m","15"]
["","Bijkomende koelmiddelvulling","","","kg/m","0,02 (voor leidinglengte van meer dan 30 m)"]
["","Totale leidinglengte","Systeem","Werkelijk","m","50"]
["Compressor","Type","","","","Hermetisch gesloten swingcompressor"]
["Afmetingen","Unit","","Breedte","mm","868"]
["","","","Diepte","mm","320"]
["","","","Hoogte","mm","734"]
["Gewicht","Unit","","","kg","57"]
["Power supply","Fase","","","","1~"]
["","Frequentie","","","Hz","50"]
["","Spanning","","","V","220-240"]
["Opmerkingen","","","","","(1) - Bevat gefluoreerde broeikasgassen"]
["","","","","","(2) - Zie afzonderlijke afbeelding voor bedrijfsbereik"]
["","","","","","(3) - Voor elektrische gegevens zie afzonderlijke tekening"]
["Ventilator-","Luchthoeveelheid","Koelen","Superlaag","m³/min","","24"]
["","","Verwarmen","Superlaag","m³/min","","24"]
["","","","Superlaag","cfm","","847"]
["","","Verwarmen","Superlaag","cfm","","847"]
["Afmetingen","Unit","","Hoogte","mm","","734"]
["","","","Breedte","mm","","868"]
["","","","Diepte","mm","","320"]
["Gewicht","Unit","","","kg","","57"]
["Ventilatormotor","Snelheid","Koelen","Superlaag","rpm","","420"]
["","","Verwarmen","Superlaag","rpm","","420"]
["Compressor","Type","","","","","Hermetisch gesloten swingcompressor"]
["Werkingsbereik","Koelen","","Min.","°CDB","","-10"]
["","","","Max.","°CDB","","46"]
["","Verwarmen","","Min.","°CWB","","-15"]
["","","","Max.","°CWB","","18"]
["Geluidsdrukniveau op 1 m","Koelen","","Nom.","dB(A)","","46"]
["","Verwarmen","","Nom.","dB(A)","","47"]
["Koelmiddel","Type","","","","","R-32"]
["","Vulling","","","kg","","1.80"]
["Koudemiddel","Vulling","","","tCO2Eq","","1.2"]
["Koelmiddel","GWP","","","","","675"]
["Koelleidingmaten","Leidinglengte","","Max.","m","","25"]
["Leidingaansluitingen","Bijkomende koelmiddelvulling","","","kg/m","","0,02 (voor leidinglengte van meer dan 30 m)"]
["Koelleidingmaten","Hoogteverschil","","Max.","m","","15"]
["","","IU - IU","Max.","m","","7.5"]
["","Totale leidinglengte","Systeem","Werkelijk","m","","50"]
["Standaard-accessoires","Installation manual","","","","","1"]
["","Drain plug","","","","","1"]
["","Screw bag","","","","","1"]
["Voeding","Fase","","","","","1~"]
["Spanningsvorm","Frequentie","","","Hz","","50"]
["","Spanning","","","V","","220-240"]