{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":43,"n_cols":8,"rows_kept":43,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","3MXM-N7"]
[]
[]
[]
[]
["","","","","","3MXM40N2V1B7","3MXM52N2V1B7","3MXM68N2V1B7"]
["Ventilator-","Luchthoeveelheid","Koelen","Superlaag","m³/min","","","24.1"]
["","","Verwarmen","Superlaag","m³/min","","","24.1"]
["","","","Superlaag","cfm","","","851"]
["","","Verwarmen","Superlaag","cfm","","","851"]
["Afmetingen","Unit","","Hoogte","mm","734","734","734"]
["","","","Breedte","mm","974","974","958"]
["","","","Diepte","mm","401","401","340"]
["Gewicht","Unit","","","kg","57","57","62"]
["Ventilatormotor","Snelheid","Koelen","Superlaag","rpm","420","420"]
["","","Verwarmen","Superlaag","rpm","420","420"]
["Compressor","Type","","","","Hermetisch gesloten swingcompressor","Hermetisch gesloten swingcompressor","Hermetisch gesloten swingcompressor"]
["Werkingsbereik","Koelen","","Min.","°C DB","-10","-10","-10"]
["","","","Max.","°C DB","46","46","46"]
["","Verwarmen","","Min.","°CWB","","","-15"]
["","","","Max.","°CWB","","","24"]
["Geluidsdrukniveau op 1 m","Koelen","","Nom.","dB(A)","46","46","48"]
["","Verwarmen","","Nom.","dB(A)","47","47","48"]
["Koelmiddel","Type","","","","R-32","R-32","R-32"]
["","Vulling","","","kg","1.8","1.8","2"]
["Koudemiddel","Vulling","","","tCO2Eq","1.22","1.22"]
["Koelmiddel","GWP","","","","675","675","675"]
["Koelleidingmaten","Leidinglengte","","Max.","m","25","25 (1)","25"]
["Leidingaansluitingen","Bijkomende koelmiddelvulling","","","kg/m","0,02 (voor leidinglengte van meer dan 30 m)","0,02 (voor leidinglengte van meer dan 30 m)","002 (voor leidinglengte van meer dan 30 m)"]
["Koelleidingmaten","Hoogteverschil","","Max.","m","15.0","15.0","15"]
["","","IU - IU","Max.","m","7.5","7.5","7.5"]
["","Totale leidinglengte","Systeem","Werkelijk","m","50","50 (2)","50"]
["Standaard-accessoires","Installation manual","","","","1","1","1"]
["","Drain cap","","","","3","3","3"]
["","Drain plug","","","","1","1","1"]
["","Reducer assembly","","","","1","1","1"]
["","Screw bag","","","","1","1","1"]
["Voeding","Fase","","","","1~","1~","1~"]
["Spanningsvorm","Frequentie","","","Hz","50","50","50"]
["","Spanning","","","V","220-240","220-240","220-440"]
["Opmerkingen","","","","","(1) - Van één kamer","(1) - Van één kamer"]
["","","","","","(2) - Voor een combinatie met CVXM-A, FVXM-A - de maximale leidinglengte is 30m.","(2) - Voor een combinatie met CVXM-A, FVXM-A - de maximale leidinglengte is 30m."]
["Bereik van het energierendement","","","","","","","A+++ ~ D"]