{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":35,"n_cols":6,"rows_kept":35,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","4MWXM-A"]
[]
[]
[]
[]
["","","","","","4MWXM52A2V1B"]
["Afmetingen","Unit","","Hoogte","mm","734"]
["","","","Breedte","mm","974"]
["","","","Diepte","mm","401"]
["Gewicht","Unit","","","kg","60"]
["Ventilatormotor","Snelheid","Koelen","Superlaag","tpm","420"]
["","","Verwarmen","Superlaag","tpm","420"]
["Compressor","Type","","","","Hermetisch gesloten swingcompressor"]
["Werkingsbereik","Koelen","","Min.","°CDB","-10"]
["","","","Max.","°CDB","46"]
["Geluidsdrukniveau op 1 m","Koelen","","Nom.","dB(A)","46"]
["","Verwarmen","","Nom.","dB(A)","47"]
["Koelmiddel","Type","","","","R-32"]
["","Vulling","","","kg","2.2"]
["Koudemiddel","Vulling","","","tCO2Eq","1.49"]
["Koelmiddel","GWP","","","","675"]
["Koelleidingmaten","Leidinglengte","","Max.","m","25 (1)"]
["Leidingaansluitingen","Bijkomende koelmiddelvulling","","","kg/m","0,02 (voor leidinglengte van meer dan 30 m)"]
["Koelleidingmaten","Hoogteverschil","","Max.","m","15.0"]
["","","IU - IU","Max.","m","7.5"]
["","Totale leidinglengte","Systeem","Werkelijk","m","50"]
["Standaard-accessoires","Installation manual","","","","1"]
["","Drain cap","","","","3"]
["","Drain plug","","","","1"]
["","Reducer assembly","","","","1"]
["","Screw bag","","","","1"]
["Voeding","Fase","","","","1~"]
["Spanningsvorm","Frequentie","","","Hz","50"]
["","Spanning","","","V","220-240"]
["Opmerkingen","","","","","(1) - Van één kamer"]