{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":6,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","5MXM-M"]
[]
[]
[]
[]
["","","","","","5MXM90M2V1B"]
["Ventilator-","Luchthoeveelheid","Koelen","Superlaag","m³/min","24.1"]
["","","Verwarmen","Superlaag","m³/min","24.1"]
["","","","Superlaag","cfm","851"]
["","","Verwarmen","Superlaag","cfm","851"]
["Afmetingen","Unit","","Hoogte","mm","734"]
["","","","Breedte","mm","320"]
["","","","Diepte","mm","868"]
["Gewicht","Unit","","","kg","68"]
["Compressor","Type","","","","Hermetisch gesloten swingcompressor"]
["Werkingsbereik","Koelen","","Min.","°CDB","-10"]
["","","","Max.","°CDB","46"]
["","Verwarmen","","Min.","°CWB","-15"]
["","","","Max.","°CWB","18"]
["Geluidsdrukniveau op 1 m","Koelen","","Nom.","dB(A)","52"]
["","Verwarmen","","Nom.","dB(A)","52"]
["Koelmiddel","Type","","","","R-32"]
["","Vulling","","","kg","2.4"]
["Koudemiddel","Vulling","","","tCO2Eq","1.6"]
["Koelmiddel","GWP","","","","675"]
["Koelleidingmaten","Leidinglengte","","Max.","m","25"]
["Leidingaansluitingen","Bijkomende koelmiddelvulling","","","kg/m","0,02 (voor leidinglengte van meer dan 30 m)"]
["Koelleidingmaten","Hoogteverschil","","Max.","m","15"]
["","","IU - IU","Max.","m","7.5"]
["","Totale leidinglengte","Systeem","Werkelijk","m","75"]
["Standaard-accessoires","Installation manual","","","","1"]
["","Drain cap","","","","9"]
["","Drain plug","","","","1"]
["","Reducer assembly","","","","1"]
["","Screw bag","","","","1"]
["Voeding","Fase","","","","1~"]
["Spanningsvorm","Frequentie","","","Hz","50"]
["","Spanning","","","V","220-240"]