{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":6,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ABQ-C / AZQS-BY1"]
[]
[]
[]
[]
["","","","","ABQ100CV1 / AZQS100B7Y1B","ABQ125CV1 / AZQS125B7Y1B"]
["Totale koelcapaciteit","Nom.","","kW","9.5","12.1 (1)"]
["Koeling","SEER","","","4.65","4.68"]
["","Jaarlijks energieverbruik","","kWu/a","716","1,550"]
["","Vermogen","Pdesign","kW","9.50","12.1"]
["","Energieklasse","","","B"]
["Verwarming (gematigd klimaat)","Vermogen","Pdesign","kW","6.78","8.13"]
["","SCOP/A","","","3.80","3.41"]
["","Energieklasse","","","A"]
["","Jaarlijks energieverbruik","","kWu/a","2,498","3,340"]
["Nominaal energierendement","Jaarlijks energieverbruik","","kWh","1,813"]
["","EER","","","2.62","2.27 (3)"]
["","COP","","","3.42"]
["","Richtlijn Energielabels","Koeling","","D"]
["","","Verwarming","","B"]
["Totale verwarmingscapaciteit","Nom.","","kW","10.8","13.5 (2)"]
["Opmerkingen","","","","(1) - EER/COP volgens Eurovent 2012, alleen voor gebruik buiten de EU","(1) - Koelen: binnentemp. 27°CDB, 19°CWB; buitentemperatuur. 35°CDB; equivalente leidinglengte: 7,5m; hoogteverschil: 0m"]
["","","","","(2) - Jaarlijks energieverbruik is conform richtlijn 2002/31/EC inzake energielabels","(2) - Verwarmen: binnentemp. 20°CDB; buitentemp. 7°CDB/6°CWB; equivalente koelmiddelleidinglengte: 7,5m; hoogteverschil: 0m"]
["","","","","(3) - SEER en SCOP zijn conform EN 14825","(3) - EER/COP volgens Eurovent 2012, alleen voor gebruik buiten de EU"]
["","","","","(4) - Nominaal rendement: koeling tegen 35°/27° nominale belasting, verwarming tegen 7°/20° nominale belasting"]