{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":9,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ADEQ-C"]
[]
[]
[]
[]
["","","","","ADEQ35C2VEB","ADEQ50C2VEB","ADEQ71C2VEB","ADEQ100C2VEB","ADEQ125C2VEB"]
["Geluidsdrukniveau op 1 m","Verwarmen","Hoog","dB(A)","37","37","31","36","38"]
["","","Nom.","dB(A)","37","37","31","36","38"]
["","","Middelhoog","dB(A)","34","34","28","33","35"]
["","","Laag","dB(A)","29","29","25","30","32"]
["","Koelen","Medium","dB(A)","32","32","28","32","35"]
["","","Laag","dB(A)","29","29","25","30","32"]
["","","Hoog","dB(A)","35","35","30","34","37"]
["","","Nom.","dB(A)","35","35","30","34","37"]
["Standaard-accessoires","Bedieningshandleiding","","","1","1","1","1","1"]
["","Montagehandleiding","","","1","1","1","1","1"]
["","Afvoerslang","","","1","1","1","1","1"]
["","Metalen klem voor afvoerslang","","","1","1","1","1","1"]
["","Sluitring voor ophangbeugel","","","8","8","8","8","8"]
["","Schroeven","","","40","40","40","40","40"]
["","Isolatie voor fitting","","","2","2","2","2","2"]
["","Afdichtingskussen","","","5","5","5","5","5"]
["","Klemmen","","","4","4","4","4","4"]
["Koudemiddel","GWP","","","2,087.5","2,087.5","2,087.5","2,087.5","2,087.5"]
["Totale koelcapaciteit","Totaalvermogen","Nom.","kW","","","","","12.10"]
["Koelleidingmaten","Vloeistof","Buitendiameter","mm","6.35","6.35","9.52","9.52","9.52"]
["","Gas","Buitendiameter","mm","9.52","12.7","15.9","15.9","15.9"]
["","Afvoer","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Sound power level","Koelen","","dB(A)","60","60","56","58","62"]
["Afmetingen","Unit","Breedte","mm","700","700","1,000","1,400","1,400"]
["","","Diepte","mm","800","800","800","800","800"]
["","","Hoogte","mm","245","245","245","245","245"]
["Behuizing","Materiaal","","","Gegalvaniseerde staalplaat","Gegalvaniseerde staalplaat","Gegalvaniseerde staalplaat","Gegalvaniseerde staalplaat","Gegalvaniseerde staalplaat"]
["","Kleur","","","Ongelakt","Ongelakt","Ongelakt","Ongelakt","Ongelakt"]
["Gewicht","Unit","","kg","28.0","28.0","35","46","46"]
["Ventilator","Externe statische druk","Hoog","Pa","150","150","150","150","150"]
["","","Nom.","Pa","30","30","30","40","50"]
["Totale verwarmingscapaciteit","Totaalvermogen","Nom.","kW","","","","","13.5"]
["Power supply","Fase","","","1~","1~","1~","1~","1~"]
["","Frequentie","","Hz","50","50","50","50","50"]
["","Spanning","","V","220-240","220-240","220-240","220-240","220-240"]
["Opmerkingen","","","","(1) - Het geluidsvermogenniveau is een absolute waarde, die het door een geluidsbron gegenereerde vermogen aangeeft.","(1) - Het geluidsvermogenniveau is een absolute waarde, die het door een geluidsbron gegenereerde vermogen aangeeft.","(1) - Het geluidsvermogenniveau is een absolute waarde, die het door een geluidsbron gegenereerde vermogen aangeeft.","(1) - Het geluidsvermogenniveau is een absolute waarde, die het door een geluidsbron gegenereerde vermogen aangeeft.","(1) - Het geluidsvermogenniveau is een absolute waarde, die het door een geluidsbron gegenereerde vermogen aangeeft."]