{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":10,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXM-A"]
[]
[]
[]
[]
["","","","","","ARXM25A5V1B","ARXM35A5V1B","ARXM50A5V1B","ARXM60A5V1B","ARXM71A5V1B"]
["Afmetingen","Unit","","Hoogte","mm","610","610","734","734","734"]
["","","","Breedte","mm","923","923","954","954","954"]
["","","","Diepte","mm","367","367","401","401","401"]
["Gewicht","Unit","","","kg","36","36","49","49","49"]
["Ventilatormotor","Snelheid","Koelen","Superlaag","rpm","600","600","500"]
["Compressor","Type","","","","Hermetisch gesloten swingcompressor","Hermetisch gesloten swingcompressor","Hermetisch gesloten swingcompressor","Hermetisch gesloten swingcompressor","Hermetisch gesloten swingcompressor"]
["Werkingsbereik","Koelen","","Min.","°C DB","-10","-10","-10","-10","-10"]
["","","","Max.","°C DB","50","50","50 (1), 46 (1)","46","46"]
["","Verwarmen","","Min.","°CWB","-21","-21","-21 (1), -15 (1)","-15","-15"]
["","","","Max.","°CWB","18","18","18","18","18"]
["Geluidsdrukniveau op 1 m","Koelen","","Nom.","dB(A)","46","47","48","48","52"]
["","Verwarmen","","Nom.","dB(A)","47","49","49","49","52"]
["Koelmiddel","Type","","","","R-32","R-32","R-32","R-32","R-32"]
["","Vulling","","","kg","0.95","0.95","1.1","1.15","1.15"]
["Koudemiddel","Vulling","","","tCO2Eq","0.65","0.65","0.75","0.78","0.78"]
["Koelmiddel","GWP","","","","675","675","675","675","675"]
["Koelleidingmaten","Leidinglengte","","Max.","m","20","20","30","30","30"]
["Leidingaansluitingen","Bijkomende koelmiddelvulling","","","kg/m","002 (voor leidinglengte van meer dan 10 m)","002 (voor leidinglengte van meer dan 10 m)","002 (voor leidinglengte van meer dan 10 m)","002 (voor leidinglengte van meer dan 10 m)","0035 (voor leidinglengte van meer dan 10m)"]
["Koelleidingmaten","Hoogteverschil","","Max.","m","15","15","20","20","20"]
["Standaard-accessoires","Installation manual","","","","1","1","1","1","1"]
["","Drain joint","","","","1","1","1"]
["","Refrigerant charge label","","","","1","1","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1","1","1"]
["","General safety precautions","","","","1","1","1"]
["","LOT10 Energy Label","","","","1","1","1"]
["","Drain cap","","","","3","3","1","3","3"]
["Bereik van het energierendement","","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Voeding","Fase","","","","1~","1~","1~","1~","1~"]
["Spanningsvorm","Frequentie","","","Hz","50","50","50","50","50"]
["","Spanning","","","V","220-240","220-240","220-240","220-240","220-240"]
["Opmerkingen","","","","","(1) - Zie afzonderlijke afbeelding voor bedrijfsbereik","(1) - Zie afzonderlijke afbeelding voor bedrijfsbereik","(1) - Zie afzonderlijke afbeelding voor bedrijfsbereik","(1) - Zie afzonderlijke afbeelding voor bedrijfsbereik","(1) - Zie afzonderlijke afbeelding voor bedrijfsbereik"]
["","","","","","(2) - Voor elektrische gegevens zie afzonderlijke tekening","(2) - Voor elektrische gegevens zie afzonderlijke tekening","(2) - Voor elektrische gegevens zie afzonderlijke tekening","(2) - Voor elektrische gegevens zie afzonderlijke tekening","(2) - Voor elektrische gegevens zie afzonderlijke tekening"]
["","","","","","(3) - Bevat gefluoreerde broeikasgassen","(3) - Bevat gefluoreerde broeikasgassen","(3) - Bevat gefluoreerde broeikasgassen","(3) - Bevat gefluoreerde broeikasgassen","(3) - Bevat gefluoreerde broeikasgassen"]
["Standaard-accessoires","ARXM50A5V1B","","","","","","1"]
["","Drain plug","","","","","","","1","1"]