{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":43,"n_cols":6,"rows_kept":43,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXL-JV"]
[]
[]
[]
[]
["","","","","ATXL25J2V1B","ATXL35J2V1B"]
["Geluidsdrukniveau op 1 m","Verwarmen","Hoog","dB(A)","41","41"]
["","","Fluisterstille werking","dB(A)","26","26"]
["","","Laag","dB(A)","29","29"]
["","Koelen","Fluisterstille werking","dB(A)","23","23"]
["","","Laag","dB(A)","27","27"]
["","","Hoog","dB(A)","41","41"]
["","","Nom.","dB(A)","35","35"]
["","Koelen","Nom.","dB(A)","34","34"]
["Standaard-accessoires","Montagehandleiding","","","1","1"]
["","Bedieningshandleiding","","","1","1"]
["","Infrarood-afstandsbediening","","","1","1"]
["","Batterijen","","","2","2"]
["","Afstandsbedieningshouder","","","1","1"]
["","Montageplaat","","","1","1"]
["","Fotokatalytisch luchtzuiveringsfilter uit titaniumapatiet","","","2","2"]
["","Montageschroeven binnenunit","","","2","2"]
["Besturingssystemen","Infrared remote control","","","ARC433A87","ARC433A87"]
["Koelleidingmaten","Vloeistof","Buitendiameter","mm","6.35","6.35"]
["","Gas","Buitendiameter","mm","9.5","9.5"]
["","Afvoer","","","18","18"]
["Opgenomen vermogen","Koelen","Nom.","kW","0.040 (2), 0.040 (3), 0.040 (4)","0.040 (2), 0.040 (3), 0.040 (4)"]
["","Verwarmen","Nom.","kW","0.040 (2), 0.040 (3), 0.040 (4)","0.040 (2), 0.040 (3), 0.040 (4)"]
["Sound power level","Koelen","","dB(A)","57","57"]
["","Verwarmen","","dB(A)","57","57"]
["Afmetingen","Unit","Breedte","mm","770","770"]
["","","Diepte","mm","198","198"]
["","","Hoogte","mm","283","283"]
["Behuizing","Kleur","","","Wit","Wit"]
["Gewicht","Unit","","kg","8","8"]
["Power supply","Fase","","","1~","1~"]
["","Frequentie","","Hz","50","50"]
["","Naam","","","V1","V1"]
["","Spanning","","V","220-240","220-240"]
["Opmerkingen","","","","(1) - Wanneer aangesloten op een multisysteem buitenunit, raadpleeg dan de karakteristieken van de multibuitenunit die aangesloten moet worden.","(1) - Wanneer aangesloten op een multisysteem buitenunit, raadpleeg dan de karakteristieken van de multibuitenunit die aangesloten moet worden."]
["","","","","(2) - 220V","(2) - 220V"]
["","","","","(3) - 230V","(3) - 230V"]
["","","","","(4) - 240V","(4) - 240V"]