{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":8,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXM-A / ARXM-A9"]
[]
[]
[]
[]
["","","","","ATXM35A2V1B / ARXM35A5V1B9","ATXM35A5V1B / ARXM35A5V1B9","ATXM50A2V1B / ARXM50A5V1B9","ATXM50A5V1B / ARXM50A5V1B9"]
["Totale koelcapaciteit","Min.","","kW","0.9","0.9","1.7","1.7"]
["","Nom.","","kW","3.5","3.5","5","5"]
["","Max.","","kW","4.4","4.4","5.3","5.3"]
["Totale verwarmingscapaciteit","Min.","","kW","0.8","0.8","1.7","1.7"]
["","Nom.","","kW","4","4","5.8","5.8"]
["","Max.","","kW","5.5","5.5","6.5","6.5"]
["Nominaal rendement","EER","","","4.5","4.5","3.58","3.58"]
["","COP","","","4.45","4.45","4.05","4.05"]
["","Jaarlijks energieverbruik","","kWu","389","389","698","698"]
["Nominaal energierendement","Richtlijn Energielabels","Koeling","","A","A","A","A"]
["","","Verwarming","","A","A","A","A"]
["Koeling","Koeling-=-Energieklasse","","","A+++","A+++","A++","A++"]
["","Vermogen","Pdesign","kW","3.5","3.5","5","5"]
["","SEER","","","9.1","9.1","7.65","7.65"]
["","Jaarlijks energieverbruik","","kWu/a","135","135","229","229"]
["Verwarming (gematigd klimaat)","Energieklasse","","","A+++","A+++","A++","A++"]
["","Vermogen","Pdesign","kW","2.5","2.5","4.5","4.5"]
["","SCOP/A","","","5.15","5.15","4.75","4.75"]
["","Pdh-verwarmingsvermogen bij -10 °C","","kW","2.5","2.5","4.5","4.5"]
["","Jaarlijks energieverbruik","","kWu/a","679","679","1326","1326"]
["Opmerkingen","","","","(1) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(2) - De nominale koelcapaciteiten zijn gebaseerd op: binnentemperatuur: 27°CDB/19°CNB, buitentemp.: 35°CDB; equivalente koelmiddelleidinglengte: 5m, hoogteverschil: 0 m.","(2) - De nominale koelcapaciteiten zijn gebaseerd op: binnentemperatuur: 27°CDB/19°CNB, buitentemp.: 35°CDB; equivalente koelmiddelleidinglengte: 5m, hoogteverschil: 0 m.","(2) - De nominale koelcapaciteiten zijn gebaseerd op: binnentemperatuur: 27°CDB/19°CNB, buitentemp.: 35°CDB; equivalente koelmiddelleidinglengte: 5m, hoogteverschil: 0 m.","(2) - De nominale koelcapaciteiten zijn gebaseerd op: binnentemperatuur: 27°CDB/19°CNB, buitentemp.: 35°CDB; equivalente koelmiddelleidinglengte: 5m, hoogteverschil: 0 m."]
["","","","","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range"]
["","","","","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data"]