{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":20,"n_cols":6,"rows_kept":20,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXM-N / ARXM-M9"]
[]
[]
[]
[]
["","","","","ATXM25N2V1B / ARXM25M3V1B9","ATXM35N2V1B / ARXM35M3V1B9"]
["Totale koelcapaciteit","Min.","","kW","1.3","1.4"]
["","Max.","","kW","3.2","4.0"]
["","Nom.","","kW","2.5","3.4"]
["Nominaal energierendement","Jaarlijks energieverbruik","","kWu","285","415"]
["","EER","","","4.39","4.09"]
["","COP","","","5.00","4.04"]
["","Richtlijn Energielabels","Koeling","","A","A"]
["","","Verwarming","","A","A"]
["Totale verwarmingscapaciteit","Nom.","","kW","2.80","4.00"]
["","Min.","","kW","1.30","1.40"]
["","Max.","","kW","4.70","5.20"]
["Opmerkingen","","","","(1) - Voor elektrische gegevens zie afzonderlijke tekening","(1) - Voor elektrische gegevens zie afzonderlijke tekening"]
["","","","","(2) - De nominale koelcapaciteiten zijn gebaseerd op: binnentemperatuur: 27°CDB/19°CNB, buitentemperatuur: 35°CDB; equivalente koelmiddelleidinglengte: 5m, hoogteverschil: 0 m.","(2) - De nominale koelcapaciteiten zijn gebaseerd op: binnentemperatuur: 27°CDB/19°CNB, buitentemperatuur: 35°CDB; equivalente koelmiddelleidinglengte: 5m, hoogteverschil: 0 m."]
["","","","","(3) - Nominale verwarmingscapaciteiten gebaseerd op: binnentemperatuur: 20°CDB, buitentemperatuur: 7°CDB/6°CWB, equivalente koelmiddelleidinglengte: 5m, hoogteverschil: 0m.","(3) - Nominale verwarmingscapaciteiten gebaseerd op: binnentemperatuur: 20°CDB, buitentemperatuur: 7°CDB/6°CWB, equivalente koelmiddelleidinglengte: 5m, hoogteverschil: 0m."]