{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":95,"n_cols":13,"rows_kept":95,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXM-R"]
[]
[]
[]
[]
["","","","","","ATXM20R2V1B §$ ATXM20R5V1B","ATXM20R2V1B (Archived)","ATXM20R5V1B (Archived)","ATXM25R2V1B (Archived)","ATXM25R5V1B (Archived)","ATXM35R2V1B (Archived)","ATXM35R5V1B (Archived)","ATXM50R2V1B (Archived)"]
["Geluidsdrukniveau op 1 m","Verwarmen","","Hoog","dB(A)","39"]
["","","","Middelhoog","dB(A)","34"]
["","","","Fluisterstille werking","dB(A)","20"]
["","","","Laag","dB(A)","26"]
["","Koelen","","Middelhoog","dB(A)","33"]
["","","","Fluisterstille werking","dB(A)","19"]
["","","","Laag","dB(A)","25"]
["","","","Hoog","dB(A)","41"]
["Standaard-accessoires","Montagehandleiding","","","","1"]
["","Bedieningshandleiding","","","","1"]
["","Draadloze afstandsbediening","","","","1"]
["","AAA drogecelbatterij","","","","2"]
["","Afstandsbedieningshouder","","","","1"]
["","Montageplaat","","","","1"]
["","Geurfilter van titaniumapatiet","","","","1"]
["","Montageschroeven binnenunit","","","","2"]
["","W-LAN-adapterkit","","","","1"]
["Regelsystemen","Bedrade afstandsbediening","","","","BRC073A1"]
["","Infrared remote control","","","","ARC466A67"]
["Leidingaansluitingen","Vloeistof","","Buitendiameter","mm","6.35"]
["","Gas","","Buitendiameter","mm","9.50"]
["","Afvoer","","","","18"]
["Opgenomen vermogen","Koelen","","Nom.","kW","0.029"]
["","Verwarmen","","Nom.","kW","0.023"]
["Sound power level","Koelen","","","dB(A)","58"]
["","Verwarmen","","","dB(A)","55"]
["Afmetingen","Unit","","Breedte","mm","778"]
["","","","Diepte","mm","272"]
["","","","Hoogte","mm","295"]
["Behuizing","Kleur","","","","Wit"]
["Gewicht","Unit","","","kg","10.0"]
["Ventilator","Luchthoeveelheid","Verwarmen","Hoog","m³/min","9.3"]
["","","","Middelhoog","m³/min","8.2"]
["","","","Laag","m³/min","6.2"]
["","","","Fluisterstille werking","m³/min","5.1"]
["","","Koelen","Laag","m³/min","5.7"]
["","","","Middelhoog","m³/min","7.5"]
["","","","Hoog","m³/min","10.5"]
["","","","Fluisterstille werking","m³/min","4.3"]
["Power supply","Fase","","","","1~"]
["","Naam","","","","V1"]
["","Frequentie","","","Hz","50"]
["","Spanning","","","V","220-240"]
["Opmerkingen","","","","","(1) - Koelen: binnentemp. 27°CDB, 19,0°CNB, buitentemp. 35°CDB, 24°CWB; equivalente leidinglengte: 5m","(1) - Koelen: binnentemp. 27°CDB, 19,0°CNB, buitentemp. 35°CDB, 24°CWB; equivalente leidinglengte: 5m","(1) - Koelen: binnentemp. 27°CDB, 19,0°CNB, buitentemp. 35°CDB, 24°CWB; equivalente leidinglengte: 5m","(1) - Koelen: binnentemp. 27°CDB, 19,0°CNB, buitentemp. 35°CDB, 24°CWB; equivalente leidinglengte: 5m","(1) - Koelen: binnentemp. 27°CDB, 19,0°CNB, buitentemp. 35°CDB, 24°CWB; equivalente leidinglengte: 5m","(1) - Koelen: binnentemp. 27°CDB, 19,0°CNB, buitentemp. 35°CDB, 24°CWB; equivalente leidinglengte: 5m","(1) - Koelen: binnentemp. 27°CDB, 19,0°CNB, buitentemp. 35°CDB, 24°CWB; equivalente leidinglengte: 5m","(1) - Verwarmen: binnentemp. 20°CDB; buitentemp. 7°CDB/6°CWB; equivalente koelmiddelleidinglengte: 5m"]
["","","","","","(2) - Verwarmen: binnentemp. 20°CDB; buitentemp. 7°CDB/6°CWB; equivalente koelmiddelleidinglengte: 5m","(2) - Verwarmen: binnentemp. 20°CDB; buitentemp. 7°CDB/6°CWB; equivalente koelmiddelleidinglengte: 5m","(2) - Verwarmen: binnentemp. 20°CDB; buitentemp. 7°CDB/6°CWB; equivalente koelmiddelleidinglengte: 5m","(2) - Verwarmen: binnentemp. 20°CDB; buitentemp. 7°CDB/6°CWB; equivalente koelmiddelleidinglengte: 5m","(2) - Verwarmen: binnentemp. 20°CDB; buitentemp. 7°CDB/6°CWB; equivalente koelmiddelleidinglengte: 5m","(2) - Verwarmen: binnentemp. 20°CDB; buitentemp. 7°CDB/6°CWB; equivalente koelmiddelleidinglengte: 5m","(2) - Verwarmen: binnentemp. 20°CDB; buitentemp. 7°CDB/6°CWB; equivalente koelmiddelleidinglengte: 5m","(2) - Koelen: binnentemp. 27°CDB, 19,0°CNB, buitentemp. 35°CDB, 24°CWB; equivalente leidinglengte: 5m"]
["Opgenomen vermogen","Koelen","","Nom.","kW","","0.029","0.029","0.029","0.029","0.03","0.03","0.03"]
["","Verwarmen","","Nom.","kW","","0.023","0.023","0.022","0.022","0.027","0.027","0.032"]
["Behuizing","Kleur","","","","","Wit","Wit","Wit","Wit","Wit","Wit","Wit"]
["Afmetingen","Unit","","Hoogte","mm","","295","295","295","295","295","295","299"]
["","","","Breedte","mm","","778","778","778","778","778","778","998"]
["","","","Diepte","mm","","272","272","272","272","272","272","292"]
["Gewicht","Unit","","","kg","","10","10","10","10","10","10","14.5"]
["Ventilator-","Luchthoeveelheid","Koelen","Hoog","m³/min","","10.5","10.5","10.5","10.5","11.3","11.3","15.8"]
["Ventilator","Luchtdebiet","Koeling","Middelhoog","m³/min","","7.5","7.5","7.6","7.6","7.8","7.8","14"]
["Ventilator-","Luchthoeveelheid","Koelen","Laag","m³/min","","5.7","5.7","5.7","5.7","6","6","11.4"]
["","","","Fluisterstille werking","m³/min","","4.3","4.3","4.1","4.1","4.2","4.2","8.3"]
["","","Verwarmen","Hoog","m³/min","","9.3","9.3","9.8","9.8","9.8","9.8","15.8"]
["Ventilator","Luchtdebiet","Verwarming","Middelhoog","m³/min","","8.2","8.2","8","8","8.5","8.5","14.2"]
["Ventilator-","Luchthoeveelheid","Verwarmen","Laag","m³/min","","6.2","6.2","6.3","6.3","6.5","6.5","12"]
["","","","Fluisterstille werking","m³/min","","5.1","5.1","4.9","4.9","4.9","4.9","10.5"]
["Geluidsvermogenniveau","Koelen","","","dB(A)","","58","58","58","58","58","58","58"]
["","Verwarmen","","","dB(A)","","55","55","55","55","55","55","58"]
["Geluidsdrukniveau op 1 m","Koelen","","Hoog","dB(A)","","41","41","41","41","45","45","44"]
["Geluidsdrukniveau","Koeling","","Middelhoog","dB(A)","","33","33","33","33","33","33","40"]
["Geluidsdrukniveau op 1 m","Koelen","","Laag","dB(A)","","25","25","25","25","25","25","36"]
["","","","Fluisterstille werking","dB(A)","","19","19","19","19","19","19","27"]
["","Verwarmen","","Hoog","dB(A)","","39","39","39","39","39","39","43"]
["Geluidsdrukniveau","Verwarming","","Middelhoog","dB(A)","","34","34","34","34","35","35","39"]
["Geluidsdrukniveau op 1 m","Verwarmen","","Laag","dB(A)","","26","26","27","27","28","28","34"]
["","","","Geluidsdrukniveau op 1 m-=-Verwarmen-=-Fluisterstille werking-=-dBA","dB(A)","","20","20","20","20","20","20","31"]
["Leidingaansluitingen","Vloeistof","","Buitendiameter","mm","","6.35","6.35","6.35","6.35","6.35","6.35","6.35"]
["","Gas","","Buitendiameter","mm","","9.5","9.5","9.5","9.5","9.5","9.5","12.7"]
["","Drainage","","","","","18","18","18","18","18","18","18"]
["Regelsystemen","IR-afstandsbediening","","","","","ARC466A67","ARC466A67","ARC466A67","ARC466A67","ARC466A67","ARC466A67","ARC466A67"]
["","Bedrade afstandsbediening","","","","","BRC073A1","BRC073A1","BRC073A1","BRC073A1","BRC073A1","BRC073A1","BRC073A1"]
["Standaard-accessoires","Installation manual","","","","","1","1","1","1","1","1","1"]
["","Wireless remote control","","","","","1","1","1","1","1","1","1"]
["","AAA dry-cell batteries","","","","","2","2","2","2","2","2","2"]
["","WLAN adapter kit","","","","","1","1","1","1","1","1","1"]
["","Operation manual","","","","","1","1","1","1","1","1","1"]
["","Titanium apatite deodorizing filter","","","","","1","1","1","1","1","1","2"]
["","Indoor unit fixing screws","","","","","2","2","2","2","2","2","2"]
["","Mounting plate","","","","","1","1","1","1","1","1","1"]
["","Remote control holder","","","","","1","1","1","1","1","1","1"]
["Voeding","Naam","","","","","V1","V1","V1","V1","V1","V1","V1"]
["","Fase","","","","","1~","1~","1~","1~","1~","1~","1~"]
["Spanningsvorm","Frequentie","","","Hz","","50","50","50","50","50","50","50"]
["","Spanning","","","V","","220-240","220-240","220-240","220-240","220-240","220-240","220-240"]
["Standaard-accessoires","Silver particle filter","","","","","","","","","","","1"]