{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":52,"n_cols":8,"rows_kept":52,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXP-N9"]
[]
[]
[]
[]
["","","","","","ATXP20N5V1B9","ATXP25N5V1B9","ATXP35N5V1B9"]
["Opgenomen vermogen","Koelen","","Nom.","kW","0.019","0.020","0.032"]
["","Verwarmen","","Nom.","kW","0.023","0.023","0.032"]
["Behuizing","Colour","","","","Wit","Wit","Wit"]
["Afmetingen","Unit","","Hoogte","mm","286","286","286"]
["","","","Breedte","mm","770","770","770"]
["","","","Diepte","mm","225","225","225"]
["Gewicht","Unit","","","kg","8.50","8.50","9.00"]
["Ventilator","Luchthoeveelheid","Koelen","Hoog","m³/min","9.5","9.7","11.5"]
["","","","Medium","m³/min","7.4","7.7","8.3"]
["","","","Laag","m³/min","5.6","5.8","6.3"]
["","","","Fluisterstille werking","m³/min","4.2","4.2","4.5"]
["","","Verwarmen","Hoog","m³/min","10.4","10.4","11.5"]
["","","","Medium","m³/min","8.1","8.1","9.0"]
["","","","Laag","m³/min","6.2","6.4","7.0"]
["","","","Fluisterstille werking","m³/min","5.2","5.2","5.1"]
["Geluidsvermogenniveau","Koelen","","","dB(A)","55","55","58"]
["","Verwarmen","","","dB(A)","55","55","58"]
["Geluidsdrukniveau op 1 m","Koelen","","Hoog","dB(A)","39","40","43"]
["","","","Medium","dB(A)","33","33","34"]
["","","","Laag","dB(A)","25","26","27"]
["","","","Fluisterstille werking","dB(A)","19","19","20"]
["","Verwarmen","","Hoog","dB(A)","39","40","40"]
["","","","Middelhoog","dB(A)","34","34","35"]
["","","","Laag","dB(A)","28","28","29"]
["","","","Fluisterstille werking","dB(A)","21","21","21"]
["Piping connections","Vloeistof","","Buitendiameter","mm","6","6","6"]
["","Gas","","Buitendiameter","mm","9.50","9.50","9.50"]
["","Afvoer","","","","18","18","18"]
["Regelsystemen","Infrared remote control","","","","ARC480A78","ARC480A78","ARC480A78"]
["","Wired remote control","","","","BRC073A1","BRC073A1","BRC073A1"]
["Standaard-accessoires","Montagehandleiding","","","","1","1","1"]
["","Bedieningshandleiding","","","","1","1","1"]
["","Infrarood-afstandsbediening","","","","1","1","1"]
["","AAA drogecelbatterij","","","","2","2","2"]
["","Afstandsbedieningshouder","","","","1","1","1"]
["","Montageplaat","","","","1","1","1"]
["","Geurfilter van titaniumapatiet","","","","1","1","1"]
["","Zilverpartikelfilter","","","","1","1","1"]
["","Montageschroeven binnenunit","","","","2","2","2"]
["","Algemene voorzorgsmaatregelen","","","","1","1","1"]
["Power supply","Phase","","","","1~","1~","1~"]
["","Frequentie","","","Hz","50","50","50"]
["","Spanning","","","V","220-240","220-240","220-240"]
["Opmerkingen","","","","","(1) - Koelen: binnentemp. 27°CDB, 19°CWB; buitentemperatuur. 35°CDB; equivalente leidinglengte: 5 m; hoogteverschil: 0m","(1) - Koelen: binnentemp. 27°CDB, 19°CWB; buitentemperatuur. 35°CDB; equivalente leidinglengte: 5 m; hoogteverschil: 0m","(1) - Koelen: binnentemp. 27°CDB, 19°CWB; buitentemperatuur. 35°CDB; equivalente leidinglengte: 5 m; hoogteverschil: 0m"]
["","","","","","(2) - Verwarmen: binnentemp. 20°CDB; buitentemp. 7°CDB/6°CWB; equivalente koelmiddelleidinglengte: 5 m (horizontaal)","(2) - Verwarmen: binnentemp. 20°CDB; buitentemp. 7°CDB/6°CWB; equivalente koelmiddelleidinglengte: 5 m (horizontaal)","(2) - Verwarmen: binnentemp. 20°CDB; buitentemp. 7°CDB/6°CWB; equivalente koelmiddelleidinglengte: 5 m (horizontaal)"]
["","","","","","(3) - Voor elektrische gegevens zie afzonderlijke tekening","(3) - Voor elektrische gegevens zie afzonderlijke tekening","(3) - Voor elektrische gegevens zie afzonderlijke tekening"]