{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":9,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","AZAS-MV1"]
[]
[]
[]
[]
["","","","","","AZAS71M2V1B","AZAS100M7V1B (Archived)","AZAS125M7V1B (Archived)","AZAS140M7V1B (Archived)"]
["Afmetingen","Unit","","Hoogte","mm","770","990","990","990"]
["","","","Breedte","mm","900","940","940","940"]
["","","","Diepte","mm","320","320","320","320"]
["Gewicht","Unit","","","kg","60","70","70","78"]
["Compressor","Type","","","","Hermetisch gesloten swingcompressor","Hermetisch gesloten swingcompressor","Hermetisch gesloten swingcompressor","Hermetisch gesloten swingcompressor"]
["Werkingsbereik","Koelen","","Min.","°CDB","-5","-5","-5","-5"]
["","","","Max.","°CDB","46","46","46","46"]
["","Verwarmen","","Min.","°CWB","-15","-15","-15","-15"]
["","","","Max.","°CWB","15.5","15.5","15.5","15.5"]
["Geluidsvermogenniveau","Koelen","","","dB(A)","65","70","71","73"]
["","Verwarmen","","","dB(A)","","","71 (1)","73 (1)"]
["Geluidsdrukniveau op 1 m","Koelen","","Nom.","dB(A)","46","53","53","54"]
["","Verwarmen","","Nom.","dB(A)","47","57","57","57"]
["Koelmiddel","Type","","","","R-32","R-32","R-32","R-32"]
["","Vulling","","","kg","2.45","2.60","2.60","2.90"]
["","GWP","","","","675","675","675","675"]
["Koudemiddel","Vulling","","","tCO2Eq","1.65","1.76","1.76","1.96"]
["Leidingaansluitingen","Vloeistof","","Buitendiameter","mm","9.52","9.52","9.52","9.52"]
["","Gas","","Buitendiameter","mm","15.9","15.9","15.9","15.9"]
["Koelleidingmaten","Leidinglengte","","Max.","m","30","30","30","30"]
["","","Systeem","Equivalent","m","50","50","50","50"]
["","","Voorgevuld tot","","m","30","30","30","30"]
["Leidingaansluitingen","Bijkomende koelmiddelvulling","","","kg/m","Zie installatiehandleiding","Zie installatiehandleiding","Zie installatiehandleiding","Zie installatiehandleiding"]
["Koelleidingmaten","Hoogteverschil","","Max.","m","30.0","30.0","30.0","30.0"]
["","","IU - IU","Max.","m","0.5","0.5","0.5","0.5"]
["Standaard-accessoires","Installation manual","","","","1","1","1","1"]
["","Refrigerant label for F-gas regulation","","","","1","1","1","1"]
["","General safety precautions","","","","1","1","1","1"]
["","LOT10 Energy Label","","","","1","1","1","1"]
["","Tie-wraps","","","","2","2","2","2"]
["Voeding","Fase","","","","1~","1~","1~","1~"]
["Spanningsvorm","Frequentie","","","Hz","50","50","50","50"]
["","Spanning","","","V","220-240","220-240","220-240","220-240"]
["Stroom: 50 Hz","Maximaal zekeringamperage (MFA)","","","A","20","25","32","32"]
["Standaard-accessoires","Peel off F-gas label","","","","1"]
["Opmerkingen","","","","","","","(1) - Volgens ENER Lot 21","(1) - Volgens ENER Lot 21"]