{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":48,"n_cols":8,"rows_kept":48,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","AZAS-MY1"]
[]
[]
[]
[]
["","","","","","AZAS125M7Y1B","AZAS100M7Y1B (Archived)","AZAS140M7Y1B (Archived)"]
["Afmetingen","Unit","","Hoogte","mm","990","990","990"]
["","","","Breedte","mm","940","940","940"]
["","","","Diepte","mm","320","320","320"]
["Gewicht","Unit","","","kg","70"]
["Compressor","Type","","","","Hermetisch gesloten swingcompressor","Hermetisch gesloten swingcompressor","Hermetisch gesloten swingcompressor"]
["Werkingsbereik","Koelen","","Min.","°C DB","-5","-5","-5"]
["","","","Max.","°C DB","46","46","46"]
["","Verwarmen","","Min.","°CWB","-15","-15","-15"]
["","","","Max.","°CWB","15.5","15.5","15.5"]
["Geluidsvermogenniveau","Koelen","","","dB(A)","71","70","73"]
["","Verwarmen","","","dB(A)","71","","73 (1)"]
["Geluidsdrukniveau op 1 m","Koelen","","Geluidsdrukniveau op 1 m-=-Koelen-=-Nom.-=-dB(A)","dB(A)","53"]
["","Verwarmen","","Geluidsdrukniveau op 1 m-=-Verwarmen-=-Nom.-=-dB(A)","dB(A)","57"]
["Koelmiddel","Type","","","","R-32","R-32","R-32"]
["Koudemiddel","Koudemiddel-=-Inhoud-=-kg","","","kg","2.60"]
["Koudemiddel","GWP","","","","675"]
["Koudemiddel","Vulling","","","tCO2Eq","1.76","1.76","1.96"]
["Leidingaansluitingen","Vloeistof","","Buitendiameter","mm","9.52","9.52","9.52"]
["Leidingaansluitingen","Gas","","Buitendiameter","mm","15.9"]
["Koelleidingmaten","Leidinglengte","","Max.","m","30","30","30"]
["","","Systeem","Equivalent","m","50","50","50"]
["","","Voorgevuld tot","","m","30","30","30"]
["Leidingaansluitingen","Bijkomende koelmiddelvulling","","","kg/m","Zie installatiehandleiding","Zie installatiehandleiding","Zie installatiehandleiding"]
["Koelleidingmaten","Hoogteverschil","","Max.","m","30.0","30.0","30.0"]
["","","IU - IU","Max.","m","0.5","0.5","0.5"]
["Standaard-accessoires","Installation manual","","","","1","1","1"]
["","Refrigerant label for F-gas regulation","","","","1","1","1"]
["","General safety precautions","","","","1","1","1"]
["","LOT10 Energy Label","","","","1","1","1"]
["","Tie-wraps","","","","2","2","2"]
["Voeding","Fase","","","","3~","3~","3~"]
["Spanningsvorm","Spanningsvorm-=-Frequentie","","Frequentie","","50","50","50"]
["","Spanningsvorm-=-Spanning","","Spanning","","380-415","380-415","380-415"]
["Stroom - 50Hz","Stroom - 50Hz-=-Afzekerwaarde","","Stroom - 50Hz-=-Afzekerwaarde-=-A","","16"]
["Opmerkingen","","","","","(1) - Volgens ENER Lot 21","","(1) - Volgens ENER Lot 21"]
["Gewicht","Unit","","","kg","","70","77"]
["Geluidsdrukniveau op 1 m","Koelen","","Nom.","dB(A)","","53","54"]
["","Verwarmen","","Nom.","dB(A)","","57","57"]
["Koelmiddel","Vulling","","","kg","","2.60","2.90"]
["","GWP","","","","","675","675"]
["Leidingaansluitingen","Gas","","Buitendiameter","mm","","15.9","15.9"]
["Stroom: 50 Hz","Maximaal zekeringamperage (MFA)","","","A","","16","16"]