{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":6,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","BRC1HHDK"]
[]
[]
[]
[]
["","","","","BRC1HHDAK (Archived)","BRC1HHDAKA (Archived)"]
["Behuizing","Kleur","","","Zwart","Zwart"]
["Omkasting","Deksel knop","","","Nee","Nee"]
["","Bedrijfs LED","Kleur","","Blauwe statusindicator","Blauwe statusindicator"]
["Afmetingen","Unit","Hoogte","mm","85","85"]
["","","Breedte","mm","85","85"]
["","","Diepte","mm","25","25"]
["","Verpakte unit","Hoogte","mm","50","50"]
["","","Breedte","mm","217","217"]
["","","Diepte","mm","161","161"]
["Gewicht","Unit","","kg","0.110","0.110"]
["","Verpakte unit","","kg","0.317","0.317"]
["Verpakking","Materiaal","","","Karton","Karton"]
["","Gewicht","","kg","0.0850","0.0850"]
["LCD","Type","","","100 x 150 dots","100 x 150 dots"]
["","Afmetingen","H","mm","40.7","40.7"]
["","","B","mm","28.0","28.0"]
["","Achtergrondverlichting","Kleur","","Wit","Wit"]
["Omgevingstemperatuur","Bedrijf","Min.","°C","-10","-10"]
["","","Max.","°C","50","50"]
["","Bewaring","Min.","°C","-20","-20"]
["","","Max.","°C","70","70"]
["","Omgevingstemperatuur-=-Relatieve vochtigheid <-=-%","","%","95","95"]
["Besturingssystemen","Klasse van temperatuurregeling","","","VI","VI"]
["","Bijdrage tot seizoensrendement van verwarming","","%","4.0","4.0"]
["Kabelaansluitingen","Lengte bekabeling","Max.","m","500","500"]