{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":8,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CHYHBH-AV32"]
[]
[]
[]
[]
["","","","","","CHYHBH05AAV32","CHYHBH05AFV32","CHYHBH08AFV32"]
["Behuizing","Kleur","","","","Wit","Wit","Wit"]
["","Materiaal","","","","Voorgelakte metaalplaat","Voorgelakte metaalplaat","Voorgelakte metaalplaat"]
["Afmetingen","Unit","","Hoogte","mm","902","902","902"]
["","","","Breedte","mm","450","450","450"]
["","","","Diepte","mm","164","164","164"]
["Gewicht","Unit","","","kg","30.0","30.0","30.0"]
["PED (richtlijn drukapparatuur)","Categorie","","","","","Art3§3, Valt buiten PED-richtlijn wegens artikel 1, punt 3.6 van 97/23/EC.","Art3§3, Valt buiten PED-richtlijn wegens artikel 1, punt 3.6 van 97/23/EC."]
["Warmtewisselaar waterzijde","Waterhoeveelheid","Verwarmen","Max.","l/min","23.0 (5)","23.0 (5)","23.0 (5)"]
["Geluidsvermogenniveau","Nom.","","","dB(A)","42 (6)","42 (6)","42 (6)"]
["Werkingsbereik","Verwarmen","waterzijdig","Min.","°C","25 (7)","25 (7)","25 (7)"]
["","","","Max.","°C","50 (7)","50 (7)","50 (7)"]
["Voeding","Naam","","","","V3","V3","V3"]
["","Fase","","","","1~","1~","1~"]
["Spanningsvorm","Frequentie","","","Hz","50","50","50"]
["","Spanning","","","V","230","230","230"]
["Kabelaansluitingen","Voor aansluiting met gebruikersinterface","","Aantal","","2","2","2"]
["","","","Opmerking","","0,75 mm² tot 1,25 mm² (max. lengte 500 m)","0,75 mm² tot 1,25 mm² (max. lengte 500 m)","0,75 mm² tot 1,25 mm² (max. lengte 500 m)"]
["Opmerkingen","","","","","(1) - Uitsluitend voor binnenunit","(1) - Uitsluitend voor binnenunit","(1) - Uitsluitend voor binnenunit"]
["","","","","","(2) - DB/NB 7°C/6°C: uitgaand water condensor 35°C (DT=5°C), boiler overbrugd","(2) - DB/NB 7°C/6°C: uitgaand water condensor 35°C (DT=5°C), boiler overbrugd","(2) - DB/NB 7°C/6°C: uitgaand water condensor 35°C (DT=5°C), boiler overbrugd"]
["","","","","","(3) - DB/NB 7°C/6°C: uitgaand water condensor 45℃ (DT=5°C), boiler overbrugd","(3) - DB/NB 7°C/6°C: uitgaand water condensor 45℃ (DT=5°C), boiler overbrugd","(3) - DB/NB 7°C/6°C: uitgaand water condensor 45℃ (DT=5°C), boiler overbrugd"]
["","","","","","(4) - Min. required","(4) - Min. required","(4) - Min. required"]
["","","","","","(5) - Boiler overbrugd","(5) - Boiler overbrugd","(5) - Boiler overbrugd"]
["","","","","","(6) - Overeenkomstig EN14825","(6) - Overeenkomstig EN14825","(6) - Overeenkomstig EN14825"]
["","","","","","(7) - Voor het bedrijfsbereik van *HYHB* en *HYKOMB33AA, zie tekening met bedrijfsbereik","(7) - Voor het bedrijfsbereik van *HYHB* en *HYKOMB33AA, zie tekening met bedrijfsbereik","(7) - Voor het bedrijfsbereik van *HYHB* en *HYKOMB33AA, zie tekening met bedrijfsbereik"]