{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":19,"n_cols":7,"rows_kept":19,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CKHWS-BV3"]
[]
[]
[]
[]
["","","","","","CKHWS180BJV3","CKHWS230BJV3"]
["Afmetingen","Unit","H","Tank","mm","1655","1855"]
["","","","Breedte","mm","595","595"]
["","","","Diepte","mm","634","634"]
["Gewicht","Unit","","Leeg","kg","106","115"]
["Tank","Watervolume","","","l","180","230"]
["","Materiaal","","","","Roestvrij staal (EN 1.4521)","Roestvrij staal (EN 1.4521)"]
["","Maximumwatertemperatuur","","","°C","65.0","65.0"]
["","Energie-efficiëntieklasse","","","","B","B"]
["Hulpverwarming","Vermogen","","","kW","1.5","1.5"]
["Opmerkingen","","","","","(1) - Gebaseerd op dT van 45 K","(1) - Gebaseerd op dT van 45 K"]
["","","","","","(2) - Stroom sanitair warm water","(2) - Stroom sanitair warm water"]
["","","","","","(3) - 2-polig 10 A, curve 230 V","(3) - 2-polig 10 A, curve 230 V"]
["","","","","","(4) - De hierboven vermelde voeding voor de hydrokit is enkel voor de back-upverwarmer. Het aansluitblok en de pomp van de hydrokit worden geleverd via de buitenunit.","(4) - De hierboven vermelde voeding voor de hydrokit is enkel voor de back-upverwarmer. Het aansluitblok en de pomp van de hydrokit worden geleverd via de buitenunit."]