{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":6,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXA-BS"]
[]
[]
[]
[]
["","","","","","CTXA15B2V1BS"]
["Opgenomen vermogen","Koelen","","Nom.","kW","0.02"]
["","Verwarmen","","Nom.","kW","0.02"]
["Behuizing","Kleur","","","","Zilver"]
["Afmetingen","Unit","","Hoogte","mm","295"]
["","","","Breedte","mm","798"]
["","","","Diepte","mm","189"]
["Gewicht","Unit","","","kg","11.5"]
["Ventilator-","Luchthoeveelheid","Koelen","Hoog","m³/min","11"]
["Ventilator","Luchtdebiet","Koeling","Middelhoog","m³/min","8.2"]
["Ventilator-","Luchthoeveelheid","Koelen","Laag","m³/min","6.1"]
["","","","Fluisterstille werking","m³/min","4.6"]
["","","Verwarmen","Hoog","m³/min","10.9"]
["Ventilator","Luchtdebiet","Verwarming","Middelhoog","m³/min","8.7"]
["Ventilator-","Luchthoeveelheid","Verwarmen","Laag","m³/min","6.4"]
["","","","Fluisterstille werking","m³/min","4.5"]
["Geluidsvermogenniveau","Koelen","","","dB(A)","57"]
["Geluidsdrukniveau op 1 m","Koelen","","Geluidsdrukniveau op 1 m-=-Koelen-=-Hoog-=-dB(A)","dB(A)","39"]
["Geluidsdrukniveau","Koeling","","Middelhoog","dB(A)","32"]
["Geluidsdrukniveau op 1 m","Koelen","","Geluidsdrukniveau op 1 m-=-Koelen-=-Laag-=-dB(A)","dB(A)","25"]
["","","","Geluidsdrukniveau op 1 m-=-Koelen-=-Fluisterstille werking-=-dB(A)","dB(A)","21"]
["","Verwarmen","","Geluidsdrukniveau op 1 m-=-Verwarmen-=-Hoog-=-dB(A)","dB(A)","39"]
["Geluidsdrukniveau","Verwarming","","Middelhoog","dB(A)","32"]
["Geluidsdrukniveau op 1 m","Verwarmen","","Geluidsdrukniveau op 1 m-=-Verwarmen-=-Laag-=-dB(A)","dB(A)","25"]
["","","","Geluidsdrukniveau op 1 m-=-Verwarmen-=-Fluisterstille werking-=-dB(A)","dB(A)","21"]
["Koelmiddel","GWP","","","","675"]
["Leidingaansluitingen","Vloeistof","","Buitendiameter","mm","6.35"]
["","Gas","","Buitendiameter","mm","9.5"]
["","Drainage","","","","18"]
["Regelsystemen","IR-afstandsbediening","","","","ARC466A58"]
["","Bedrade afstandsbediening","","","","BRC073"]
["Standaard-accessoires","Installation manual","","","","1"]
["","Screw cover","","","","2"]
["","AAA dry-cell batteries","","","","2"]
["","General safety precautions","","","","1"]
["","Operation manual","","","","1"]
["","Luchtfilter","","","","2"]
["","Infrared remote control","","","","1"]
["","Remote controller mounting plate","","","","1"]
["","Screw bag","","","","1"]
["Voeding","Naam","","","","V1"]
["","Fase","","","","1~"]
["Spanningsvorm","Frequentie","","","Hz","50"]
["","Spanning","","","V","220-240"]