{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":6,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXA-BT"]
[]
[]
[]
[]
["","","","","","CTXA15B2V1BT"]
["Geluidsdrukniveau op 1 m","Verwarmen","","Hoog","dB(A)","39"]
["","","","Middelhoog","dB(A)","32"]
["","","","Fluisterstille werking","dB(A)","21"]
["","","","Laag","dB(A)","25"]
["","Koelen","","Medium","dB(A)","32"]
["","","","Fluisterstille werking","dB(A)","21"]
["","","","Laag","dB(A)","25"]
["","","","Hoog","dB(A)","39"]
["Standaard-accessoires","Montagehandleiding","","","","1"]
["","Bedieningshandleiding","","","","1"]
["","Luchtfilter","","","","2"]
["","Infrarood-afstandsbediening","","","","1"]
["","Montageplaat afstandsbediening","","","","1"]
["","Zakje schroeven","","","","1"]
["","Schroefdeksel","","","","2"]
["","AAA drogecelbatterij","","","","2"]
["","Algemene voorzorgsmaatregelen","","","","1"]
["Koudemiddel","GWP","","","","675.0"]
["Besturingssystemen","Wired remote control","","","","BRC073"]
["","Infrared remote control","","","","ARC466A58"]
["Koelleidingmaten","Vloeistof","","Buitendiameter","mm","6.35"]
["","Gas","","Buitendiameter","mm","9.50"]
["","Afvoer","","","","18"]
["Opgenomen vermogen","Koelen","","Nom.","kW","0.020"]
["","Verwarmen","","Nom.","kW","0.020"]
["Sound power level","Koelen","","","dB(A)","57"]
["Afmetingen","Unit","","Breedte","mm","798"]
["","","","Diepte","mm","189"]
["","","","Hoogte","mm","295"]
["Behuizing","Kleur","","","","Zwart hout"]
["Gewicht","Unit","","","kg","11.5"]
["Ventilator","Luchthoeveelheid","Verwarmen","Hoog","m³/min","10.9"]
["","","","Medium","m³/min","8.7"]
["","","","Laag","m³/min","6.4"]
["","","","Fluisterstille werking","m³/min","4.5"]
["","","Koelen","Laag","m³/min","6.1"]
["","","","Medium","m³/min","8.2"]
["","","","Hoog","m³/min","11.0"]
["","","","Fluisterstille werking","m³/min","4.6"]
["Power supply","Fase","","","","1~"]
["","Naam","","","","V1"]
["","Frequentie","","","Hz","50"]
["","Spanning","","","V","220-240"]