{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":6,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXF-F / 2MXF-A"]
[]
[]
[]
[]
["","","","","CTXF20F5V1B / CTXF20F5V1B / 2MXF40A2V1B","CTXF25F5V1B / CTXF25F5V1B / 2MXF50A2V1B"]
["Totale koelcapaciteit","Min.","","kW","1.5","1.8"]
["","Nom.","","kW","4","5"]
["","Max.","","kW","4.2","5.3"]
["Totale verwarmingscapaciteit","Min.","","kW","1.3","1.2"]
["","Nom.","","kW","4.2","5.6"]
["","Max.","","kW","4.6","5.8"]
["Nominaal rendement","EER","","","3.9","3.37"]
["","COP","","","4.1","3.71"]
["","Jaarlijks energieverbruik","","kWu","513","742"]
["Nominaal energierendement","Richtlijn Energielabels","Koeling","","A","A"]
["","","Verwarming","","A","A"]
["Koeling","Koeling-=-Energieklasse","","","A++","A++"]
["","Vermogen","Pdesign","kW","4","5"]
["","SEER","","","7.5","7.85"]
["","Jaarlijks energieverbruik","","kWu/a","187","223"]
["Verwarming (gematigd klimaat)","Energieklasse","","","A+","A+"]
["","Vermogen","Pdesign","kW","3.2","4.2"]
["","SCOP/A","","","4.3","4.31"]
["","Pdh-verwarmingsvermogen bij -10 °C","","kW","2.46","3.32"]
["","Jaarlijks energieverbruik","","kWu/a","1043","1364"]