{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":50,"n_cols":7,"rows_kept":50,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXF-F"]
[]
[]
[]
[]
["","","","","","CTXF25F5V1B (Archived)","CTXF35F5V1B (Archived)"]
["Opgenomen vermogen","Koelen","","Nom.","kW","0.023","0.029"]
["","Verwarmen","","Nom.","kW","0.023","0.023"]
["Behuizing","Kleur","","","","Wit","Wit"]
["Afmetingen","Unit","","Hoogte","mm","286","286"]
["","","","Breedte","mm","770","770"]
["","","","Diepte","mm","225","225"]
["Gewicht","Unit","","","kg","8.5","9"]
["Ventilator-","Luchthoeveelheid","Koelen","Hoog","m³/min","9.8","10.9"]
["Ventilator","Luchtdebiet","Koeling","Middelhoog","m³/min","8","7"]
["Ventilator-","Luchthoeveelheid","Koelen","Laag","m³/min","6","5.7"]
["","","","Fluisterstille werking","m³/min","4.3","4.6"]
["","","Verwarmen","Hoog","m³/min","10.4","9.3"]
["Ventilator","Luchtdebiet","Verwarming","Middelhoog","m³/min","8.4","7.5"]
["Ventilator-","Luchthoeveelheid","Verwarmen","Laag","m³/min","6.4","6"]
["","","","Fluisterstille werking","m³/min","5.3","5.2"]
["Geluidsvermogenniveau","Koelen","","","dB(A)","54","54"]
["","Verwarmen","","","dB(A)","55","56"]
["Geluidsdrukniveau op 1 m","Koelen","","Hoog","dB(A)","40","56"]
["Geluidsdrukniveau","Koeling","","Middelhoog","dB(A)","33"]
["Geluidsdrukniveau op 1 m","Koelen","","Laag","dB(A)","26"]
["","","","Fluisterstille werking","dB(A)","20"]
["","Verwarmen","","Hoog","dB(A)","40","40"]
["Geluidsdrukniveau","Verwarming","","Middelhoog","dB(A)","34","35"]
["Geluidsdrukniveau op 1 m","Verwarmen","","Laag","dB(A)","28","29"]
["","","","Geluidsdrukniveau op 1 m-=-Verwarmen-=-Fluisterstille werking-=-dBA","dB(A)","21","21"]
["Leidingaansluitingen","Vloeistof","","Buitendiameter","mm","6","6"]
["","Gas","","Buitendiameter","mm","9.5","9.5"]
["","Drainage","","","","18","18"]
["Regelsystemen","IR-afstandsbediening","","","","ARC480A93","ARC480A93"]
["","Bedrade afstandsbediening","","","","BRC073A1","BRC073A1"]
["Standaard-accessoires","Installation manual","","","","1","1"]
["","AAA dry-cell batteries","","","","2","2"]
["","General safety precautions","","","","1","1"]
["","Operation manual","","","","1","1"]
["","Indoor unit fixing screws","","","","2","2"]
["","Infrared remote control","","","","1","1"]
["","Mounting plate","","","","1","1"]
["","Remote control holder","","","","1","1"]
["Voeding","Fase","","","","1~","1~"]
["Spanningsvorm","Frequentie","","","Hz","50","50"]
["","Spanning","","","V","220-440","220-440"]
["Opmerkingen","","","","","(1) - Koelen: binnentemp. 27°CDB, 19°CWB; buitentemperatuur. 35°CDB; equivalente leidinglengte: 5 m; hoogteverschil: 0m","(1) - Koelen: binnentemp. 27°CDB, 19°CWB; buitentemperatuur. 35°CDB; equivalente leidinglengte: 5 m; hoogteverschil: 0m"]
["","","","","","(2) - Verwarmen: binnentemp. 20°CDB; buitentemp. 7°CDB/6°CWB; equivalente koelmiddelleidinglengte: 5 m (horizontaal)","(2) - Verwarmen: binnentemp. 20°CDB; buitentemp. 7°CDB/6°CWB; equivalente koelmiddelleidinglengte: 5 m (horizontaal)"]
["","","","","","(3) - Voor elektrische gegevens zie afzonderlijke tekening","(3) - Voor elektrische gegevens zie afzonderlijke tekening"]