{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":6,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXM-R / 5MXM-N9"]
[]
[]
[]
[]
["","","","","CTXM15R2V1B / FTXM71R2V1B / 5MXM90N2V1B9","CTXM15R5V1B / FTXM71R2V1B / 5MXM90N2V1B9"]
["Koelcapaciteit","Nom.","","kW","8.00","8.00"]
["Koeling","SEER","","","6.84","6.84"]
["","Jaarlijks energieverbruik","","kWu/a","410","410"]
["","Vermogen","Pdesign","kW","8.00","8.00"]
["","Energieklasse","","","A+++","A+++"]
["Verwarming (gematigd klimaat)","Vermogen","Pdesign","kW","4.50","4.50"]
["","SCOP/A","","","4.28","4.28"]
["","Energieklasse","","","A+","A+"]
["","Jaarlijks energieverbruik","","kWu/a","1,472","1,472"]
["Nominaal energierendement","Jaarlijks energieverbruik","","kWh","1,202","1,202"]
["","EER","","","3.33","3.33"]
["","COP","","","3.67","3.67"]
["","Richtlijn Energielabels","Koeling","","A","A"]
["","","Verwarming","","A","A"]
["Totale verwarmingscapaciteit","Nom.","","kW","10.00","10.00"]
["Opmerkingen","","","","(1) - De nominale koelcapaciteiten zijn gebaseerd op: binnentemperatuur: 27°CDB/19°CNB, buitentemp.: 35°CDB; equivalente koelmiddelleidinglengte: 5m, hoogteverschil: 0 m.","(1) - De nominale koelcapaciteiten zijn gebaseerd op: binnentemperatuur: 27°CDB/19°CNB, buitentemp.: 35°CDB; equivalente koelmiddelleidinglengte: 5m, hoogteverschil: 0 m."]
["","","","","(2) - Nominale verwarmingscapaciteiten gebaseerd op: binnentemperatuur: 20°CDB, buitentemperatuur: 7°CDB/6°CWB, equivalente koelmiddelleidinglengte: 5m, hoogteverschil: 0m.","(2) - Nominale verwarmingscapaciteiten gebaseerd op: binnentemperatuur: 20°CDB, buitentemperatuur: 7°CDB/6°CWB, equivalente koelmiddelleidinglengte: 5m, hoogteverschil: 0m."]
["","","","","(3) - Zie afzonderlijke afbeelding voor bedrijfsbereik","(3) - Zie afzonderlijke afbeelding voor bedrijfsbereik"]
["","","","","(4) - Voor elektrische gegevens zie afzonderlijke tekening","(4) - Voor elektrische gegevens zie afzonderlijke tekening"]