{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":29,"n_cols":13,"rows_kept":29,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EBSXB-D"]
[]
[]
[]
[]
["","","","","","EBSXB11P50DG","EBSXB11P30DG","EBSXB16P50DG","EBSXB16P30DG","EBSXB11P30DF (Archived)","EBSXB11P50DF (Archived)","EBSXB16P30DF (Archived)","EBSXB16P50DF (Archived)"]
["Behuizing","Kleur","","","","Wit (RAL9016) / Zwart (RAL9017)","Wit (RAL9016) / Zwart (RAL9017)","Wit (RAL9016) / Zwart (RAL9017)","Wit (RAL9016) / Zwart (RAL9017)","Wit (RAL9016) / Zwart (RAL9017)","Wit (RAL9016) / Zwart (RAL9017)","Wit (RAL9016) / Zwart (RAL9017)","Wit (RAL9016) / Zwart (RAL9017)"]
["","Materiaal","","","","Slagvast polypropyleen","Slagvast polypropyleen","Slagvast polypropyleen","Slagvast polypropyleen","Slagvast polypropyleen","Slagvast polypropyleen","Slagvast polypropyleen","Slagvast polypropyleen"]
["Afmetingen","Unit","","Hoogte","mm","1,910","1,893","1,910","1,893","1,893","1,910","1,893","1,910"]
["","","","Breedte","mm","792","594","792","594","594","792","594","792"]
["","","","Diepte","mm","817","680","817","680","680","817","680","817"]
["Gewicht","Unit","","","kg","117","94","117","94","94","117","94","117"]
["PED (richtlijn drukapparatuur)","Categorie","","","","Categorie II","Categorie II","Categorie II","Categorie II","Categorie II","Categorie II","Categorie II","Categorie II"]
["Koelmiddel","Type","","","","R-32","R-32","R-32","R-32","R-32","R-32","R-32","R-32"]
["","GWP","","","","675.0","675.0","675.0","675.0","675.0","675.0","675.0","675.0"]
["","Vulling","","","kg","3.80","3.80","3.80","3.80","3.80","3.80","3.80","3.80"]
["Koudemiddel","Vulling","","","tCO2Eq","2.57","2.57","2.57","2.57","2.57","2.57","2.57","2.57"]
["Geluidsvermogenniveau","Nom.","","","dB(A)","44.7","44.7","49.0","49.0","44.7","44.7","49.0","49.0"]
["Geluidsdrukniveau op 1 m","Nom.","","","dB(A)","36.8","36.8","40.3","40.3","36.8","36.8","40.3","40.3"]
["Werkingsbereik","Verwarmen","waterzijdig","Min.","°C","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)"]
["","","","Max.","°C","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)"]
["","Koelen","","Min.","°C DB","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)"]
["","","Waterzijde","Min.","°C","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)"]
["","","","Max.","°C","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)"]
["Voeding","Fase","","","","1~","1~","1~","1~","1~","1~","1~","1~"]
["Spanningsvorm","Frequentie","","","Hz","50","50","50","50","50","50","50","50"]
["","Spanning","","","V","230","230","230","230","230","230","230","230"]
["Opmerkingen","","","","","(1) - Warmteverlies volgens EN12897","(1) - Warmteverlies volgens EN12897","(1) - Warmteverlies volgens EN12897","(1) - Warmteverlies volgens EN12897","(1) - Warmteverlies volgens EN12897","(1) - Warmteverlies volgens EN12897","(1) - Warmteverlies volgens EN12897","(1) - Warmteverlies volgens EN12897"]
["","","","","","(2) - Raadpleeg de tekening met bedrijfslimieten","(2) - Raadpleeg de tekening met bedrijfslimieten","(2) - Raadpleeg de tekening met bedrijfslimieten","(2) - Raadpleeg de tekening met bedrijfslimieten","(2) - Raadpleeg de tekening met bedrijfslimieten","(2) - Raadpleeg de tekening met bedrijfslimieten","(2) - Raadpleeg de tekening met bedrijfslimieten","(2) - Raadpleeg de tekening met bedrijfslimieten"]