{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":22,"n_cols":9,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EBVH-D6V / ERLA-DW17"]
[]
[]
[]
[]
["","","","","","EBVH16S18DJ6V / ERLA16DAW17","EBVH16S23DJ6V / ERLA16DAW17","EBVH16S18DJ6V / ERLA16D2W17","EBVH16S23DJ6V / ERLA16D2W17"]
["Totale verwarmingscapaciteit","Nom.","","","kW","16.0, 16.0","16.0, 16.0","16.0 (2) (1), 16.0 (2) (1)","16.0, 16.0"]
["Opgenomen vermogen","Verwarmen","","Nom.","kW","3.53, 4.56","3.53, 4.56","3.53 (1), 4.56 (2)","3.53, 4.56"]
["","Sanitair warm water van 10°C tot 50°C","","Nom.","kWh","2.44","3.41","2.44","3.41"]
["Opwarmingstijd van 10°C tot 50°C","uur","","","","1 uur 25 minuten bij omgevingstemperatuur van 7°C","1 uur 25 minuten bij omgevingstemperatuur van 7°C","1 uur 25 minuten bij omgevingstemperatuur van 7°C","1 uur 25 minuten bij omgevingstemperatuur van 7°C"]
["COP","","","","","4.53, 3.51","4.53, 3.51","4.53 (1), 3.51 (2)","4.53, 3.51"]
["Verwarming van sanitair warm water","Algemeen","","Aangegevens belastingprofiel","","L","XL","L","XL"]
["","Gematigd klimaat","","Energierendementsklasse waterverwarming","","A+","A","A+","A"]
["Verwarming","Wateruitlaat gematigd klimaat 55°C","Algemeen","SCOP","","3.32","3.32","3.32","3.32"]
["","","","Seizoensefficiëntieklasse verwarming","","A++","A++","A++","A++"]
["","Wateruitlaat gematigd klimaat 35°C","Algemeen","SCOP","","4.61","4.61","4.61","4.61"]
["","","","Seizoensefficiëntieklasse verwarming","","A+++","A+++","A+++","A+++"]
["Opmerkingen","","","","","(1) - Voorwaarde: Ta DB/NB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Voorwaarde: Ta DB/NB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Voorwaarde: Ta DB/NB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Voorwaarde: Ta DB/NB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - Voorwaarde: Ta DB/WB 7 °C / 6 °C - LWC 45 °C (Dt=5 °C)","(2) - Voorwaarde: Ta DB/WB 7 °C / 6 °C - LWC 45 °C (Dt=5 °C)","(2) - Voorwaarde: Ta DB/WB 7 °C / 6 °C - LWC 45 °C (Dt=5 °C)","(2) - Voorwaarde: Ta DB/WB 7 °C / 6 °C - LWC 45 °C (Dt=5 °C)"]
["","","","","","(3) - Toestand 1: koelen Ta 35°C - LWE 18°C (DT = 5°C); verwarmen Ta DB/NB 7°C/6°C - LWC 35°C (DT = 5°C)","(3) - Toestand 1: koelen Ta 35°C - LWE 18°C (DT = 5°C); verwarmen Ta DB/NB 7°C/6°C - LWC 35°C (DT = 5°C)","(3) - Toestand 1: koelen Ta 35°C - LWE 18°C (DT = 5°C); verwarmen Ta DB/NB 7°C/6°C - LWC 35°C (DT = 5°C)","(3) - Toestand 1: koelen Ta 35°C - LWE 18°C (DT = 5°C); verwarmen Ta DB/NB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(4) - Toestand 2: koelen Ta 35°C - LWE 7°C (DT = 5°C); verwarmen Ta DB/NB 7°C/6°C - LWC 45°C (DT = 5°C)","(4) - Toestand 2: koelen Ta 35°C - LWE 7°C (DT = 5°C); verwarmen Ta DB/NB 7°C/6°C - LWC 45°C (DT = 5°C)","(4) - Toestand 2: koelen Ta 35°C - LWE 7°C (DT = 5°C); verwarmen Ta DB/NB 7°C/6°C - LWC 45°C (DT = 5°C)","(4) - Toestand 2: koelen Ta 35°C - LWE 7°C (DT = 5°C); verwarmen Ta DB/NB 7°C/6°C - LWC 45°C (DT = 5°C)"]
["","","","","","(5) - Gemeten bij een drukdaling van 10 kPa in het verwarmingssysteem met een uitgaande watertemperatuur van 47-55°C in een kamer met een omgevingstemperatuur van 20°C DB/WB 7°C/6°.","(5) - Gemeten bij een drukdaling van 10 kPa in het verwarmingssysteem met een uitgaande watertemperatuur van 47-55°C in een kamer met een omgevingstemperatuur van 20°C DB/WB 7°C/6°.","(5) - Gemeten bij een drukdaling van 10 kPa in het verwarmingssysteem met een uitgaande watertemperatuur van 47-55°C in een kamer met een omgevingstemperatuur van 20°C DB/WB 7°C/6°.","(5) - Gemeten bij een drukdaling van 10 kPa in het verwarmingssysteem met een uitgaande watertemperatuur van 47-55°C in een kamer met een omgevingstemperatuur van 20°C DB/WB 7°C/6°."]