{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":7,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHFH-D3V / ERLA-DV"]
[]
[]
[]
[]
["","","","","","EHFH03S18DJ3V / ERLA03DAV3","EHFH03S18DA3V / ERLA03DAV3"]
["Totale verwarmingscapaciteit","Min.","","","kW","1.26 (1)"]
["","Nom.","","","kW","3.59 (1), 3.53 (2)","3.50 (1) (2)"]
["Totale koelcapaciteit","Min.","","","kW","1.8 (1)"]
["","Nom.","","","kW","3.44 (1), 3.49 (2)"]
["Opgenomen vermogen","Verwarmen","","Nom.","kW","0.720 (1), 1.21 (2)","0.710 (1), 1.19 (2)"]
["","Koelen","","Min.","kW","0.62 (1), 1.17 (2)"]
["","Sanitair warm water van 10°C tot 50°C","","Nom.","kWh","2.58"]
["Opwarmingstijd van 10°C tot 50°C","uur","","","","1h35min"]
["COP","","","","","5.00 (1), 2.94 (2)","4.91 (1), 2.95 (2)"]
["EER","","","","","5.60 (1), 3.03 (2)"]
["Verwarming van sanitair warm water","Algemeen","","Aangegevens belastingprofiel","","L","L"]
["","Gematigd klimaat","","Energierendementsklasse waterverwarming","","A"]
["Verwarming","Wateruitlaat gematigd klimaat 55°C","Algemeen","SCOP","","3.23"]
["","","","Seizoensefficiëntieklasse verwarming","","A++"]
["","Wateruitlaat gematigd klimaat 35°C","Algemeen","SCOP","","4.40"]
["","","","Seizoensefficiëntieklasse verwarming","","A++"]
["Bereik van het energierendement","","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F"]
["Opmerkingen","","","","","(1) - Toestand 1: koelen Ta 35°C - LWE 18°C (DT = 5°C); verwarmen Ta DB/NB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Toestand 1: koelen Ta 35°C - LWE 18°C (DT = 5°C); verwarmen Ta DB/NB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - Toestand 5: Koeling Ta 35°C - LWE 7°C (DT = 5°C); Verwarming Ta DB/NB 7°C/6°C - LWC 55°C (DT = 8°C)","(2) - Toestand 5: Koeling Ta 35°C - LWE 7°C (DT = 5°C); Verwarming Ta DB/NB 7°C/6°C - LWC 55°C (DT = 8°C)"]
["","","","","","(3) - Koelen Ta 35°C - LWE 18°C ( DT = 5°C ) - Verwarmen Ta DB/WB 7°C/6°C - LWC 35°C ( DT = 5°C)"]