{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":8,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHSH-E"]
[]
[]
[]
[]
["","","","","","EHSH04P30EF (Archived)","EHSH08P30EF (Archived)","EHSH08P50EF (Archived)"]
["Behuizing","Kleur","","","","Wit (RAL9016) / Zwart (RAL9017)","Wit (RAL9016) / Zwart (RAL9017)","Wit (RAL9016) / Zwart (RAL9017)"]
["","Materiaal","","","","Slagvast polypropyleen","Slagvast polypropyleen","Slagvast polypropyleen"]
["Afmetingen","Unit","","Hoogte","mm","1,892","1,892","1,905"]
["","","","Breedte","mm","594","594","792"]
["","","","Diepte","mm","644","644","812"]
["Gewicht","Unit","","","kg","77","77","107"]
["PED (richtlijn drukapparatuur)","Categorie","","","","Art 4.3","Art 4.3","Art 4.3"]
["Koelmiddel","Type","","","","R-32","R-32","R-32"]
["","GWP","","","","675","675","675"]
["","Vulling","","","kg","1.5","1.5","1.5"]
["Geluidsvermogenniveau","Nom.","","","dB(A)","39","39","39"]
["Werkingsbereik","Verwarmen","waterzijdig","Min.","°C","18","18","18"]
["","","","Max.","°C","65","65","65"]
["","Koelen","","Min.","°CDB","10","10","10"]
["","","Waterzijde","Min.","°C","5","5","5"]
["","","","Max.","°C","22","22","22"]
["Voeding","Fase","","","","1~","1~","1~"]
["Spanningsvorm","Frequentie","","","Hz","50","50","50"]
["","Spanning","","","V","230","230","230"]
["Opmerkingen","","","","","(1) - Warmteverlies volgens EN12897","(1) - Warmteverlies volgens EN12897","(1) - Warmteverlies volgens EN12897"]