{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":19,"n_cols":9,"rows_kept":19,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHVZ-E9W / ERGA-EVH7"]
[]
[]
[]
[]
["","","","","","EHVZ08S18EA9W / ERGA08EAV3H7","EHVZ08S18EJ9W / ERGA08EAV3H7","EHVZ08S23EA9W / ERGA08EAV3H7","EHVZ08S23EJ9W / ERGA08EAV3H7"]
["Totale verwarmingscapaciteit","Nom.","","","kW","7.5 (1), 7.8 (2)","7.5 (1), 7.8 (2)","7.5 (1), 7.8 (2)","7.5 (1), 7.8 (2)"]
["Opgenomen vermogen","Verwarmen","","Nom.","kW","1.63 (1), 2.23 (2)","1.63 (1), 2.23 (2)","1.63 (1), 2.23 (2)","1.63 (1), 2.23 (2)"]
["","Sanitair warm water van 10°C tot 50°C","","Nom.","kWh","2.48","2.48","3.01","3.01"]
["Opwarmingstijd van 10°C tot 50°C","uur","","","","1u28min","1u28min","1u40min","1u40min"]
["COP","","","","","4.6 (1), 3.5 (2)","4.6 (1), 3.5 (2)","4.6 (1), 3.5 (2)","4.6 (1), 3.5 (2)"]
["Verwarming van sanitair warm water","Algemeen","","Aangegevens belastingprofiel","","L","L","XL","XL"]
["","Gematigd klimaat","","Energierendementsklasse waterverwarming","","A+","A+","A+","A+"]
["Verwarming","Wateruitlaat gematigd klimaat 55°C","Algemeen","SCOP","","3.32","3.32","3.32","3.32"]
["","","","Seizoensefficiëntieklasse verwarming","","A++","A++","A++","A++"]
["","Wateruitlaat gematigd klimaat 35°C","Algemeen","SCOP","","4.56","4.56","4.56","4.56"]
["","","","Seizoensefficiëntieklasse verwarming","","A+++","A+++","A+++","A+++"]
["Opmerkingen","","","","","(1) - Toestand 1: koelen Ta 35°C - LWE 18°C (DT = 5°C); verwarmen Ta DB/NB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Toestand 1: koelen Ta 35°C - LWE 18°C (DT = 5°C); verwarmen Ta DB/NB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Toestand 1: koelen Ta 35°C - LWE 18°C (DT = 5°C); verwarmen Ta DB/NB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Toestand 1: koelen Ta 35°C - LWE 18°C (DT = 5°C); verwarmen Ta DB/NB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - Toestand 2: koelen Ta 35°C - LWE 7°C (DT = 5°C); verwarmen Ta DB/NB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Toestand 2: koelen Ta 35°C - LWE 7°C (DT = 5°C); verwarmen Ta DB/NB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Toestand 2: koelen Ta 35°C - LWE 7°C (DT = 5°C); verwarmen Ta DB/NB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Toestand 2: koelen Ta 35°C - LWE 7°C (DT = 5°C); verwarmen Ta DB/NB 7°C/6°C - LWC 45°C (DT = 5°C)"]