{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":45,"n_cols":7,"rows_kept":45,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHY2KOMB-A"]
[]
[]
[]
[]
["","","","","","EHY2KOMB28AA","EHY2KOMB32AA"]
["Gas","Aansluiting","","Diameter","mm","15","15"]
["","Verbruik (G20)","","Min","m³/u","0.74","0.79"]
["","","","Max","m³/u","3.02","3.39"]
["","Verbruik (G25)","","Min","m³/u","0.84","0.89"]
["","","","Max","m³/u","3.46","3.92"]
["","Verbruik (G31)","","Min","m³/u","0.28","0.30"]
["","","","Max","m³/u","1.15","1.29"]
["","NOx-klasse","","","","6","6"]
["","NOx-peil (G20)","","","mg/kWu","27","36"]
["Centrale verwarming","Opgenomen warmte Qn (thermische netto-waarde)","Nom","Min","kW","7.1","7.6"]
["","","","Max","kW","23.7","27.0"]
["","Opgenomen warmte Qn (thermische bruto-waarde)","Nom","Min","kW","7.9","8.4"]
["","","","Max","kW","26.3","30.0"]
["","Uitgaand Pn bij 80/60°C","","Min","kW","7.1","7.4"]
["","","","Nom","kW","23.1","26.6"]
["","Uitgaand Pn bij 50/30°C","","Min","kW","7.7","8.2"]
["","","","Nom","kW","25.4","28.9"]
["","Rendement bij 37/30°C","","Nom","kW","7.7","8.2"]
["","Watertemperatuur","","Max","°C","90","90"]
["Sanitair warm water","Opgenomen warmte (thermische netto-waarde) Qnw","Nom","Min","kW","7.9","8.4"]
["","","","Max","kW","32.3","36.3"]
["","Comfortklasse (EN13203)","","","","XL","XL"]
["","Temperatuur","","Sanitair warm water-=-Temperatuur-=-Max-=-°C","°C","65","65"]
["Toevoerlucht","Concentrisch","","","","nee","nee"]
["Afvoergas","Temperatuur","","Max","°C","70","70"]
["","Aansluiting","","","mm","60","60"]
["","Massahoeveelheid (G20)","","Max","kg/u","48.6","54.4"]
["","Massahoeveelheid (G25)","","Max","kg/u","48.6","54.4"]
["","Massahoeveelheid (G31)","","Max","kg/u","47.9","53.6"]
["Behuizing","Kleur","","","","RAL9010","RAL9010"]
["","Materiaal","","","","Voorgelakte metaalplaat","Voorgelakte metaalplaat"]
["Afmetingen","Unit","Hoogte","Behuizing","mm","650","710"]
["","","","Breedte","mm","450","450"]
["","","","Diepte","mm","240","240"]
["Gewicht","Unit","","Leeg","kg","33","36"]
["Verwarming van sanitair warm water","Algemeen","","Aangegevens belastingprofiel","","XL","XL"]
["","","","Energierendementsklasse waterverwarming","","A","A"]
["Centrale verwarming","Algemeen","","Seizoensrendementsklasse verwarmen","","A","A"]
["Bereik van het energierendement","","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F"]