{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":6,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EJHA-AV3"]
[]
[]
[]
[]
["","","","","","EJHA04AAV3"]
["Geluidsdrukniveau op 1 m","Verwarmen","","Nom.","dB(A)","37.0"]
["Koudemiddel","GWP","","","","675.0"]
["","Vulling","","","kg","0.560"]
["","Type","","","","R-32"]
["Bedrijfsbereik","Heating","Max.","Max.","°CWB","25"]
["","Warmtapwater","Omgeving","Min.","°C DB","-14"]
["","","","Max.","°C DB","35"]
["Opgenomen vermogen","Verwarmen","","Nom.","kW","0.850 (1)"]
["Geluidsvermogenniveau","Heating","","Nom.","dB(A)","58.7"]
["COP","","","","","4.49 (1)"]
["Afmetingen","Unit","","Breedte","mm","845"]
["","","","Diepte","mm","329"]
["","","","Hoogte","mm","745"]
["Gewicht","Unit","","","kg","45.0"]
["Verwarming","Wateruitlaat gematigd klimaat 35°C","General","ηs (seizoensefficiëntie ruimteverwarming)","%","116"]
["","","","Seizoensefficiëntieklasse verwarming","","A"]
["","","","SCOP","","2.98"]
["","Wateruitlaat gematigd klimaat 55°C","Algemeen","Seasonal space heating eff. class","","A+"]
["","","","ηs (seizoensefficiëntie ruimteverwarming)","%","101"]
["","","","SCOP","","2.60"]
["Ventilator","Luchthoeveelheid","Verwarmen","Hoog","m³/min","28.3"]
["Totale verwarmingscapaciteit","Nom.","","","kW","4.53 (1)"]
["Power supply","Fase","","","","1~"]
["","Naam","","","","V3"]
["","Frequentie","","","Hz","50"]
["","Spanning","","","V","220-240"]
["Opmerkingen","","","","","(1) - Verwarmen: uitgaand water condensor 35°C; Dt 5°C; omgevingstemperatuur 7°CDB, 6°CWB"]