{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":32,"n_cols":6,"rows_kept":32,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ELBX-E6V"]
[]
[]
[]
[]
["","","","","","ELBX12EF6V"]
["Behuizing","Kleur","","","","Wilt + zwart"]
["","Materiaal","","","","Kunsthars, metaalplaat"]
["Afmetingen","Unit","","Hoogte","mm","840"]
["","","","Breedte","mm","440"]
["","","","Diepte","mm","390"]
["Gewicht","Unit","","","kg","48.5"]
["PED (richtlijn drukapparatuur)","Categorie","","","","Categorie II"]
["Geluidsvermogenniveau","Nom.","","","dB(A)","44.0"]
["Geluidsdrukniveau op 1 m","Nom.","","","dB(A)","30.0"]
["Werkingsbereik","Verwarmen","waterzijdig","Min.","°C","15"]
["","","","Max.","°C","65"]
["","Koelen","","Min.","°CDB","10"]
["","","Waterzijde","Min.","°C","5"]
["","","","Max.","°C","22"]
["Voeding","Naam","","","","Zie opmerking 6"]
["Elektrische verwarming","Spanningsvorm","","Naam","","6V3"]
["","","","Fase","","1~ / 3~"]
["","","","Frequentie","Hz","50"]
["","","","Spanning","V","230"]
["","Afzekerwaarde","","","A","20.000"]
["Opmerkingen","","","","","(1) - Het bedrijfsbereik is uitgebreid tot lagere debieten, afhankelijk van de bedrijfsmodus - raadpleeg de ESP-curve."]
["","","","","","(2) - Excluding the water volume in the unit. This volume will guarantee suficient defrost energy for all applications, however, this volume can be multiplied by 0,66 if the heating sepoint is ≥ 45° C (eg. Fan coils)"]
["","","","","","(3) - Gemeten bij een drukdaling van 10 kPa in het verwarmingssysteem met een uitgaande watertemperatuur van 47-55°C in een kamer met een omgevingstemperatuur van 20°C DB/WB 7°C/6°."]
["","","","","","(4) - Sound values are measured in a semi-anechoic room. Sound pressure level is a relative value, depending on the distance and acoustic environment. For more details, please refer to the sound level drawings. Sound power level is an absolute value that a so"]
["","","","","","(5) - Raadpleeg de werkbereik-tekening voor meer informatie"]
["","","","","","(6) - 4-polige zekering 20 A curve 400 V klasse C (zie bedradingsschema)"]