{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":9,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ELSHB-E"]
[]
[]
[]
[]
["","","","","","ELSHB12P50EG","ELSHB12P30EG","ELSHB12P30EF (Archived)","ELSHB12P50EF (Archived)"]
["Behuizing","Kleur","","","","Wit (RAL9016) / Zwart (RAL9017)","Wit (RAL9016) / Zwart (RAL9017)","Wit (RAL9016) / Zwart (RAL9017)","Wit (RAL9016) / Zwart (RAL9017)"]
["","Materiaal","","","","Slagvast polypropyleen","Slagvast polypropyleen","Slagvast polypropyleen","Slagvast polypropyleen"]
["Afmetingen","Unit","","Hoogte","mm","1,910","1,891","1,893","1,910"]
["","","","Breedte","mm","792","594","594","792"]
["","","","Diepte","mm","817","680","680","817"]
["Gewicht","Unit","","","kg","115","93.0","76.0","91.0"]
["PED (richtlijn drukapparatuur)","Categorie","","","","Categorie II","Categorie II","Categorie II","Categorie II"]
["Koelmiddel","Type","","","","R-32","R-32","R-32","R-32"]
["Geluidsvermogenniveau","Nom.","","","dB(A)","44.7","44.7","44.7","44.7"]
["Geluidsdrukniveau op 1 m","Nom.","","","dB(A)","36.8","36.8","36.8","36.8"]
["Werkingsbereik","Verwarmen","waterzijdig","Min.","°C","15 (3)","15 (3)","15 (3)","15 (3)"]
["","","","Max.","°C","65 (3)","65 (3)","65 (3)","65 (3)"]
["","Koelen","","Min.","°C DB","10 (3)","10 (3)","10 (3)","10 (3)"]
["","","Waterzijde","Min.","°C","5 (3)","5 (3)","5 (3)","5 (3)"]
["","","","Max.","°C","22 (3)","22 (3)","22 (3)","22 (3)"]
["Voeding","Fase","","","","1~","1~","1~","1~"]
["Spanningsvorm","Frequentie","","","Hz","50","50","50","50"]
["","Spanning","","","V","230","230","230","230"]
["Opmerkingen","","","","","(1) - Het bedrijfsbereik is uitgebreid tot lagere debieten, afhankelijk van de bedrijfsmodus - raadpleeg de ESP-curve.","(1) - Het bedrijfsbereik is uitgebreid tot lagere debieten, afhankelijk van de bedrijfsmodus - raadpleeg de ESP-curve.","(1) - Het bedrijfsbereik is uitgebreid tot lagere debieten, afhankelijk van de bedrijfsmodus - raadpleeg de ESP-curve.","(1) - Het bedrijfsbereik is uitgebreid tot lagere debieten, afhankelijk van de bedrijfsmodus - raadpleeg de ESP-curve."]
["","","","","","(2) - Warmteverlies volgens EN12897","(2) - Warmteverlies volgens EN12897","(2) - Warmteverlies volgens EN12897","(2) - Warmteverlies volgens EN12897"]
["","","","","","(3) - Raadpleeg de werkbereik-tekening voor meer informatie","(3) - Raadpleeg de werkbereik-tekening voor meer informatie","(3) - Raadpleeg de werkbereik-tekening voor meer informatie","(3) - Raadpleeg de werkbereik-tekening voor meer informatie"]