{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":34,"n_cols":7,"rows_kept":34,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EPSK08-10AW1"]
[]
[]
[]
[]
["","","","","","EPSK08ARW1 (Archived)","EPSK10ARW1 (Archived)"]
["Afmetingen","Unit","","Hoogte","mm","1123","1123"]
["","","","Breedte","mm","1330","1330"]
["","","","Diepte","mm","604","604"]
["Gewicht","Unit","","","kg","178","178"]
["Ventilator-","Luchthoeveelheid","Verwarmen","Hoog","m³/min","75.7","75.7"]
["","","Koelen","Hoog","m³/min","75.7","75.7"]
["Bedrijfsbereik","Koelen","","Min.","°CDB","10","10"]
["","","","Max.","°CDB","43","43"]
["Werkingsbereik","Warmtapwater","","Min.","°CDB","-28","-28"]
["Bedrijfsbereik","Sanitair warm water","","Max.","°CDB","40","40"]
["Geluidsvermogenniveau","Verwarmen","","Nom.","dB(A)","45 (1)","47 (1)"]
["","Koelen","","Nom.","dB(A)","53 (2)","53.2 (2)"]
["Geluidsdrukniveau op 1 m","Verwarmen","","Nom.","dB(A)","32.4 (1)","32.8 (1)"]
["","Koelen","","Nom.","dB(A)","37.2 (2)","37.3 (2)"]
["Koelmiddel","Type","","","","R-290","R-290"]
["","GWP","","","","3","3"]
["Koudemiddel","Vulling","","","tCO2Eq","0.003","0.003"]
["Koelmiddel","Vulling","","","kg","1","1"]
["Koelleidingmaten","Hoogteverschil","","Max.","m","10","10"]
["Voeding","Naam","","","","W1","W1"]
["","Fase","","","","3~","3~"]
["Spanningsvorm","Frequentie","","","Hz","50","50"]
["","Spanning","","","V","400","400"]
["Stroom","Stroom-=-Afzekerwaarde-=-A","","","A","16","16"]
["Opmerkingen","","","","","(1) - Gemeten bij LWC 47-55°C; Ta DB/NB 7°C/6°C.","(1) - Gemeten bij LWC 47-55°C; Ta DB/NB 7°C/6°C."]
["","","","","","(2) - Gemeten bij LWC 12-7°C; Ta 35 °C.","(2) - Gemeten bij LWC 12-7°C; Ta 35 °C."]
["","","","","","(3) - Leidingen van 1 1/4” ter plaatse","(3) - Leidingen van 1 1/4” ter plaatse"]
["","","","","","(4) - Leidingen van 1 1/2” ter plaatse","(4) - Leidingen van 1 1/2” ter plaatse"]