{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":6,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ERLA-DV"]
[]
[]
[]
[]
["","","","","","ERLA03DAV3 (Archived)"]
["Afmetingen","Unit","","Hoogte","mm","550"]
["","","","Breedte","mm","765"]
["","","","Diepte","mm","285"]
["Gewicht","Unit","","","kg","35"]
["Ventilator-","Luchthoeveelheid","Verwarmen","Hoog","m³/min","32.0"]
["","","Koelen","Hoog","m³/min","36"]
["Bedrijfsbereik","Koelen","","Min.","°C DB","10"]
["","","","Max.","°C DB","43"]
["Werkingsbereik","Warmtapwater","","Min.","°C DB","-15"]
["Bedrijfsbereik","Sanitair warm water","","Max.","°C DB","35"]
["Geluidsvermogenniveau","Verwarmen","","Nom.","dB(A)","59"]
["","Koelen","","Nom.","dB(A)","60"]
["Geluidsdrukniveau op 1 m","Verwarmen","","Nom.","dB(A)","46.0"]
["","Koelen","","Nom.","dB(A)","46"]
["Koelmiddel","Type","","","","R-32"]
["","GWP","","","","675.0"]
["Koudemiddel","Vulling","","","tCO2Eq","0.675"]
["Koelmiddel","Vulling","","","kg","1"]
["Leidingaansluitingen","Vloeistof","","Buitendiameter","mm","6.35"]
["","Gas","","Buitendiameter","mm","9.52"]
["Koelleidingmaten","Hoogteverschil","","Max.","m","20.0"]
["Voeding","Naam","","","","V3"]
["","Fase","","","","1N~"]
["Spanningsvorm","Frequentie","","","Hz","50"]
["","Spanning","","","V","220-240"]
["Stroom","Stroom-=-Afzekerwaarde-=-A","","","A","16"]
["Opmerkingen","","","","","(1) - Koelen Ta 35°C - LWE 18°C ( DT = 5°C ) - Verwarmen Ta DB/WB 7°C/6°C - LWC 35°C ( DT = 5°C)"]