{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":36,"n_cols":6,"rows_kept":36,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ERRA08-12EV3"]
[]
[]
[]
[]
["","","","","","ERRA10EAV3 (Archived)"]
["Afmetingen","Unit","","Hoogte","mm","1,003"]
["","","","Breedte","mm","1270"]
["","","","Diepte","mm","533"]
["Gewicht","Unit","","","kg","107"]
["Ventilator-","Luchthoeveelheid","Verwarmen","Hoog","m³/min","89.9"]
["","","Koelen","Hoog","m³/min","80.1"]
["Bedrijfsbereik","Koelen","","Min.","°C DB","10"]
["","","","Max.","°C DB","43"]
["Werkingsbereik","Warmtapwater","","Min.","°C DB","-25"]
["Bedrijfsbereik","Sanitair warm water","","Max.","°C DB","35"]
["Geluidsvermogenniveau","Verwarmen","","Nom.","dB(A)","56.0"]
["","Koelen","","Nom.","dB(A)","60.6"]
["Geluidsdrukniveau op 1 m","Verwarmen","","Nom.","dB(A)","40.6"]
["","Koelen","","Nom.","dB(A)","47.4"]
["Koelmiddel","Type","","","","R-32"]
["","GWP","","","","675.0"]
["Koudemiddel","Vulling","","","tCO2Eq","2.19"]
["Koelmiddel","Vulling","","","kg","3.25"]
["Leidingaansluitingen","Vloeistof","","Buitendiameter","mm","6.35"]
["","Gas","","Buitendiameter","mm","15.9"]
["Koelleidingmaten","Hoogteverschil","","Max.","m","30.0"]
["Voeding","Naam","","","","V3"]
["","Fase","","","","1~"]
["Spanningsvorm","Frequentie","","","Hz","50"]
["","Spanning","","","V","230"]
["Stroom","Stroom-=-Afzekerwaarde-=-A","","","A","32"]
["Opmerkingen","","","","","(1) - Koelen Ta 35°C - LWE 18°C ( DT = 5°C ) - Verwarmen Ta DB/WB 7°C/6°C - LWC 35°C ( DT = 5°C)"]
["","","","","","(2) - Toestand 2: koelen Ta 35°C - LWE 7°C (DT = 5°C); verwarmen Ta DB/NB 7°C/6°C - LWC 45°C (DT = 5°C)"]
["","","","","","(3) - Het geluidsdrukniveau is een relatieve waarde, die afhankelijk is van de afstand en de akoestische omgeving. Zie de geluidsniveautekeningen voor meer bijzonderheden."]
["","","","","","(4) - Het geluidsdrukniveau wordt gemeten met een microfoon op een bepaalde afstand van de unit. Het is een relatieve waarde die afhangt van de afstand en de akoestische omgeving. Raadpleeg de tekening met geluidsspectrum-gegevens voor meer informatie. Omstandigheid: Ta 35°C - LWE 7°C (DT = 5°C)"]