{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":29,"n_cols":6,"rows_kept":29,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ETBX12E6V / EPRA08-12EV"]
[]
[]
[]
[]
["","","","","","ETBX12EJ6V / EPRA10EAV3"]
["Binnendeel","","","","","ETBX12EF6V"]
["Totale verwarmingscapaciteit","Min.","","","kW","3.44 (1)"]
["","Nom.","","","kW","6.17 (2)"]
["","Max.","","","kW","9.25 (1)"]
["Totale koelcapaciteit","Nom.","","","kW","7.97 (3), 6.47 (4)"]
["Opgenomen vermogen","Verwarmen","","Min.","kW","0.72 (5)"]
["","","","Nom.","kW","1.25 (2)"]
["","","","Max.","kW","2.04 (5)"]
["","Koelen","","Nom.","kW","2.66 (3), 1.16 (4)"]
["COP","","","","","4.92 (2)"]
["EER","","","","","3.00 (3), 5.56 (4)"]
["Verwarming","Wateruitlaat gematigd klimaat 55°C","Algemeen","SCOP","","3.48"]
["","","","Seizoensefficiëntieklasse verwarming","","A++"]
["","Wateruitlaat gematigd klimaat 35°C","Algemeen","SCOP","","4.82"]
["","","","Seizoensefficiëntieklasse verwarming","","A+++"]
["Bereik van het energierendement","","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F"]
["Opmerkingen","","","","","(1) - Capaciteit overeenkomstig norm EN14511 en geldig voor een verwarmd waterbereik met dT = 3~8°C at Ta 7°C"]
["","","","","","(2) - Voorwaarde: Ta DB/NB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(3) - Koelen: EW 12°C; LW 7°C; omgevingsomstandigheden: 35°CDB"]
["","","","","","(4) - Koelen: EW 23°C; LW 18°C; omgevingsomstandigheden: 35°CDB"]
["","","","","","(5) - Het opgenomen vermogen is het totaal van binnen- en buitenunits, met inbegrip van de circulatiepomp; overeenkomstig EN14511"]
["","","","","","(6) - Getest bij Ta DB/NB 7°C/6°C. Conform EN 16147."]
["","","","","","(7) - DB/WB 7°C/6°C - LWC 35°C (dT=5°C) met pomp aan volledig toerental"]