{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":11,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ETSX16E / EPRA14-18DW7"]
[]
[]
[]
[]
["","","","","","ETSX16P50EF / EPRA14DAW17","ETSX16P30EF / EPRA14DAW17","ETSX16P50EF / EPRA16DAW17","ETSX16P30EF / EPRA16DAW17","ETSX16P30EF / EPRA18DAW17","ETSX16P50EF / EPRA18DAW17"]
["Totale verwarmingscapaciteit","Min.","","","kW","","","396.00 (1)"]
["","Nom.","","","kW","","","9.00 (2)"]
["","Max.","","","kW","","","1,044.00 (1)"]
["Totale koelcapaciteit","Nom.","","","kW","","","115 (3), 788 (4)"]
["Opgenomen vermogen","Verwarmen","","Min.","kW","","","9.00 (5)"]
["","","","Nom.","kW","","","18.0 (2)"]
["","","","Max.","kW","","","232.00 (5)"]
["","Koelen","","Nom.","kW","","","28.0 (3), 293 (4)"]
["COP","","","","","479.00","479.00","5.00 (2)","5.00","5.00","5.00"]
["EER","","","","","413.00, 27.00","413.00, 27.00","411.00 (3), 269.00 (4)","411.00, 269.00","409.00, 268.00","409.00, 268.00"]
["Sanitair warm water","Algemeen","","Aangegevens belastingprofiel","","","","XL"]
["","Gematigd klimaat","","Energierendementsklasse waterverwarming","","","","A+"]
["Verwarming","Wateruitlaat gematigd klimaat 55°C","Algemeen","SCOP","","","","3.63"]
["","","","Seasonal space heating eff. class","","","","A++"]
["","Wateruitlaat gematigd klimaat 35°C","Algemeen","SCOP","","","","4.81"]
["","","","Seizoensefficiëntieklasse verwarming","","","","A+++"]
["Opmerkingen","","","","","(1) - Capaciteit overeenkomstig norm EN14511 en geldig voor een verwarmd waterbereik met dT = 3~8°C at Ta 7°C","(1) - Capaciteit overeenkomstig norm EN14511 en geldig voor een verwarmd waterbereik met dT = 3~8°C at Ta 7°C","(1) - Capaciteit overeenkomstig norm EN14511 en geldig voor een verwarmd waterbereik met dT = 3~8°C at Ta 7°C","(1) - Capaciteit overeenkomstig norm EN14511 en geldig voor een verwarmd waterbereik met dT = 3~8°C at Ta 7°C","(1) - Capaciteit overeenkomstig norm EN14511 en geldig voor een verwarmd waterbereik met dT = 3~8°C at Ta 7°C","(1) - Capaciteit overeenkomstig norm EN14511 en geldig voor een verwarmd waterbereik met dT = 3~8°C at Ta 7°C"]
["","","","","","(2) - Voorwaarde: Ta DB/NB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Voorwaarde: Ta DB/NB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Voorwaarde: Ta DB/NB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Voorwaarde: Ta DB/NB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Voorwaarde: Ta DB/NB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Voorwaarde: Ta DB/NB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(3) - Koelen: EW 23°C; LW 18°C; omgevingsomstandigheden: 35°CDB","(3) - Koelen: EW 23°C; LW 18°C; omgevingsomstandigheden: 35°CDB","(3) - Koelen: EW 23°C; LW 18°C; omgevingsomstandigheden: 35°CDB","(3) - Koelen: EW 23°C; LW 18°C; omgevingsomstandigheden: 35°CDB","(3) - Koelen: EW 23°C; LW 18°C; omgevingsomstandigheden: 35°CDB","(3) - Koelen: EW 23°C; LW 18°C; omgevingsomstandigheden: 35°CDB"]
["","","","","","(4) - Koelen: EW 12°C; LW 7°C; omgevingsomstandigheden: 35°CDB","(4) - Koelen: EW 12°C; LW 7°C; omgevingsomstandigheden: 35°CDB","(4) - Koelen: EW 12℃; LW 7℃; omgevingsomstandigheden: 35°CDB","(4) - Koelen: EW 12°C; LW 7°C; omgevingsomstandigheden: 35°CDB","(4) - Koelen: EW 12°C; LW 7°C; omgevingsomstandigheden: 35°CDB","(4) - Koelen: EW 12°C; LW 7°C; omgevingsomstandigheden: 35°CDB"]
["","","","","","(5) - Het opgenomen vermogen is het totaal van binnen- en buitenunits, met inbegrip van de circulatiepomp; overeenkomstig EN14511","(5) - Het opgenomen vermogen is het totaal van binnen- en buitenunits, met inbegrip van de circulatiepomp; overeenkomstig EN14511","(5) - Het opgenomen vermogen is het totaal van binnen- en buitenunits, met inbegrip van de circulatiepomp; overeenkomstig EN14511","(5) - Het opgenomen vermogen is het totaal van binnen- en buitenunits, met inbegrip van de circulatiepomp; overeenkomstig EN14511","(5) - Het opgenomen vermogen is het totaal van binnen- en buitenunits, met inbegrip van de circulatiepomp; overeenkomstig EN14511","(5) - Het opgenomen vermogen is het totaal van binnen- en buitenunits, met inbegrip van de circulatiepomp; overeenkomstig EN14511"]
["Totale verwarmingscapaciteit","Min.","","","kW","37.00","37.00","","396.00","44.00","44.00"]
["","Nom.","","","kW","59.0","59.0","","9.00","9.00","9.00"]
["","Max.","","","kW","975.00","975.00","","1044.00","116.00","116.00"]
["Totale koelcapaciteit","Nom.","","","kW","106, 69.0","106, 69.0","","115, 788","125, 886","125, 886"]
["Opgenomen vermogen","Verwarmen","","Min.","kW","84.00","84.00","","9.00","1.00","1.00"]
["","","","Nom.","kW","123","123","","18.0","18.0","18.0"]
["","","","Max.","kW","217.00","217.00","","232.00","258.00","258.00"]
["","Koelen","","Nom.","kW","255, 256","255, 256","","28.0, 293","305, 331","305, 331"]
["Verwarming van sanitair warm water","Algemeen","","Aangegevens belastingprofiel","","XL","L","","L","L","XL"]
["","Gematigd klimaat","","Energierendementsklasse waterverwarming","","A+","A+","","A+","A+","A+"]
["Verwarming","Wateruitlaat gematigd klimaat 55°C","Algemeen","SCOP","","3.63","3.63","","3.63","3.63","3.63"]
["","","","Seizoensefficiëntieklasse verwarming","","A++","A++","","A++","A++","A++"]
["","Wateruitlaat gematigd klimaat 35°C","Algemeen","SCOP","","4.81","4.81","","4.81","4.81","4.81"]
["","","","Seizoensefficiëntieklasse verwarming","","A+++","A+++","","A+++","A+++","A+++"]