{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":17,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ETSXB12E / EPRA08-12EW"]
[]
[]
[]
[]
["","","","","","ETSXB12P30EF / EPRA08EAW1","ETSXB12P50EF / EPRA08EAW1","ETSXB12P30EG / EPRA08EAW1","ETSXB12P50EG / EPRA08EAW1","ETSXB12P30EF / EPRA10EAW1","ETSXB12P50EF / EPRA10EAW1","ETSXB12P30EG / EPRA10EAW1","ETSXB12P50EG / EPRA10EAW1","ETSXB12P30EF / EPRA12EAW1","ETSXB12P50EF / EPRA12EAW1","ETSXB12P30EG / EPRA12EAW1","ETSXB12P50EG / EPRA12EAW1"]
["Binnendeel","","","","","ETSXB12P30EF","ETSXB12P50EF","ETSXB12P30EG","ETSXB12P50EG","ETSXB12P30EF","ETSXB12P50EF","ETSXB12P30EG","ETSXB12P50EG","ETSXB12P30EF","ETSXB12P50EF","ETSXB12P30EG","ETSXB12P50EG"]
["Totale verwarmingscapaciteit","Nom.","","","kW","6.17 (1)","6.17 (1)","6.17 (1)","6.17 (1)","6.17 (1)","6.17 (1)","6.17 (1)","6.17 (1)","6.17 (1)","6.17 (1)","6.17 (1)","6.17 (1)"]
["Totale koelcapaciteit","Nom.","","","kW","6.81 (2)","6.81 (2)","6.81 (2)","6.81 (2)","7.97 (2)","7.97 (2)","7.97 (2)","7.97 (2)","8.62 (2)","8.62 (2)","8.62 (2)","8.62 (2)"]
["Opgenomen vermogen","Verwarmen","","Nom.","kW","1.21 (1)","1.21 (1)","1.21 (1)","1.21 (1)","1.21 (1)","1.21 (1)","1.21 (1)","1.21 (1)","1.21 (1)","1.21 (1)","1.21 (1)","1.21 (1)"]
["","Koelen","","Nom.","kW","2.08 (2)","2.08 (2)","2.08 (2)","2.08 (2)","2.57 (2)","2.57 (2)","2.57 (2)","2.57 (2)","2.86 (2)","2.86 (2)","2.86 (2)","2.86 (2)"]
["COP","","","","","5.1","5.1","5.10 (1)","5.10 (1)","5.1","5.1","5.10 (1)","5.10 (1)","5.1","5.1","5.10 (1)","5.10 (1)"]
["EER","","","","","3.28 (2)","3.28 (2)","3.28 (2)","3.28 (2)","3.1","3.1","3.10 (2)","3.10 (2)","3.01 (2)","3.01 (2)","3.01 (2)","3.01 (2)"]
["Verwarming van sanitair warm water","Algemeen","","Aangegevens belastingprofiel","","L","XL","L","XL","L","XL","L","XL","L","XL","L","XL"]
["","Gematigd klimaat","","Energierendementsklasse waterverwarming","","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+"]
["Verwarming","Wateruitlaat gematigd klimaat 55°C","Algemeen","SCOP","","3.59","3.59","3.59","3.59","3.6","3.6","3.60","3.60","3.6","3.6","3.60","3.60"]
["","","","Seizoensefficiëntieklasse verwarming","","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++"]
["","Wateruitlaat gematigd klimaat 35°C","Algemeen","SCOP","","4.95","4.95","4.95","4.95","4.98","4.98","4.98","4.98","4.98","4.98","4.98","4.98"]
["","","","Seizoensefficiëntieklasse verwarming","","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++"]
["Bereik van het energierendement","","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F"]
["Opmerkingen","","","","","(1) - Toestand 1: koelen Ta 35°C - LWE 18°C (DT = 5°C); verwarmen Ta DB/NB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Toestand 1: koelen Ta 35°C - LWE 18°C (DT = 5°C); verwarmen Ta DB/NB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Toestand 1: koelen Ta 35°C - LWE 18°C (DT = 5°C); verwarmen Ta DB/NB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Toestand 1: koelen Ta 35°C - LWE 18°C (DT = 5°C); verwarmen Ta DB/NB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Toestand 1: koelen Ta 35°C - LWE 18°C (DT = 5°C); verwarmen Ta DB/NB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Toestand 1: koelen Ta 35°C - LWE 18°C (DT = 5°C); verwarmen Ta DB/NB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Toestand 1: koelen Ta 35°C - LWE 18°C (DT = 5°C); verwarmen Ta DB/NB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Toestand 1: koelen Ta 35°C - LWE 18°C (DT = 5°C); verwarmen Ta DB/NB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Toestand 1: koelen Ta 35°C - LWE 18°C (DT = 5°C); verwarmen Ta DB/NB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Toestand 1: koelen Ta 35°C - LWE 18°C (DT = 5°C); verwarmen Ta DB/NB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Toestand 1: koelen Ta 35°C - LWE 18°C (DT = 5°C); verwarmen Ta DB/NB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Toestand 1: koelen Ta 35°C - LWE 18°C (DT = 5°C); verwarmen Ta DB/NB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - Toestand 2: koelen Ta 35°C - LWE 7°C (DT = 5°C); verwarmen Ta DB/NB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Toestand 2: koelen Ta 35°C - LWE 7°C (DT = 5°C); verwarmen Ta DB/NB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Toestand 2: koelen Ta 35°C - LWE 7°C (DT = 5°C); verwarmen Ta DB/NB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Toestand 2: koelen Ta 35°C - LWE 7°C (DT = 5°C); verwarmen Ta DB/NB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Toestand 2: koelen Ta 35°C - LWE 7°C (DT = 5°C); verwarmen Ta DB/NB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Toestand 2: koelen Ta 35°C - LWE 7°C (DT = 5°C); verwarmen Ta DB/NB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Toestand 2: koelen Ta 35°C - LWE 7°C (DT = 5°C); verwarmen Ta DB/NB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Toestand 2: koelen Ta 35°C - LWE 7°C (DT = 5°C); verwarmen Ta DB/NB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Toestand 2: koelen Ta 35°C - LWE 7°C (DT = 5°C); verwarmen Ta DB/NB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Toestand 2: koelen Ta 35°C - LWE 7°C (DT = 5°C); verwarmen Ta DB/NB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Toestand 2: koelen Ta 35°C - LWE 7°C (DT = 5°C); verwarmen Ta DB/NB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Toestand 2: koelen Ta 35°C - LWE 7°C (DT = 5°C); verwarmen Ta DB/NB 7°C/6°C - LWC 45°C (DT = 5°C)"]
["","","","","","(3) - DB/WB 7°C/6°C - LWC 35°C (dT=5°C) met pomp aan volledig toerental","(3) - DB/WB 7°C/6°C - LWC 35°C (dT=5°C) met pomp aan volledig toerental","(3) - DB/WB 7°C/6°C - LWC 35°C (dT=5°C) met pomp aan volledig toerental","(3) - DB/WB 7°C/6°C - LWC 35°C (dT=5°C) met pomp aan volledig toerental","(3) - DB/WB 7°C/6°C - LWC 35°C (dT=5°C) met pomp aan volledig toerental","(3) - DB/WB 7°C/6°C - LWC 35°C (dT=5°C) met pomp aan volledig toerental","(3) - DB/WB 7°C/6°C - LWC 35°C (dT=5°C) met pomp aan volledig toerental","(3) - DB/WB 7°C/6°C - LWC 35°C (dT=5°C) met pomp aan volledig toerental","(3) - DB/WB 7°C/6°C - LWC 35°C (dT=5°C) met pomp aan volledig toerental","(3) - DB/WB 7°C/6°C - LWC 35°C (dT=5°C) met pomp aan volledig toerental","(3) - DB/WB 7°C/6°C - LWC 35°C (dT=5°C) met pomp aan volledig toerental","(3) - DB/WB 7°C/6°C - LWC 35°C (dT=5°C) met pomp aan volledig toerental"]