{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":48,"n_cols":8,"rows_kept":48,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EWAA-DW1P-H"]
[]
[]
[]
[]
["","","","","","EWAA011DAW1P-H-","EWAA014DAW1P-H-","EWAA016DAW1P-H-"]
["Geluidsdrukniveau op 1 m","Koelen","","Nom.","dB(A)","47.7","50.8","51.0"]
["Hydraulische componenten","Expansievat","","Volume","l","8","8","8"]
["Werkingsbereik","Luchtzijdig","Koelen","Min.","°C DB","10","10","10"]
["","","","Max.","°C DB","43","43","43"]
["","Waterkant","Koelen","Max.","°C DB","22","22","22"]
["","","","Min.","°C DB","5","5","5"]
["Koelmiddelvolume","Per circuit","","","kg","3.80","3.80","3.80"]
["","Refrigerant charge-=-Per circuit-=-TCO2Eq","","","tCO2eq","2.6","2.6","2.6"]
["Compressor","Type","","","","Hermetisch gesloten swing-inverter-compressor","Hermetisch gesloten swing-inverter-compressor","Hermetisch gesloten swing-inverter-compressor"]
["","Aanloopmethode_","","","","Invertergestuurd","Invertergestuurd","Invertergestuurd"]
["","Aantal_","","","","1","1","1"]
["Luchtgekoelde warmtewisselaar","Type","","","","Uiterst efficiënte lamel en buistype met integrale nakoeler","Uiterst efficiënte lamel en buistype met integrale nakoeler","Uiterst efficiënte lamel en buistype met integrale nakoeler"]
["Gewicht","Unit","","","kg","147","147","147"]
["EER","","","","","3.26 (1), 5.31 (2)","3.16 (1), 5.04 (2)","3.06 (1), 4.74 (2)"]
["Koudemiddel","GWP","","","","675.0","675.0","675.0"]
["","Type","","","","R-32","R-32","R-32"]
["","Circuits","","Aantal","","1","1","1"]
["","Regeling","","","","Elektronische expansieklep","Elektronische expansieklep","Elektronische expansieklep"]
["Ventilatormotor","Snelheid","Koelen","Nom.","rpm","550","650","650"]
["Totale koelcapaciteit","Nom.","","","kW","11.6 (1), 11.5 (2)","12.8 (1), 12.7 (2)","14.0 (1), 15.3 (2)"]
["Warmtewisselaar","Watervolume","","","l","2","2","2"]
["","Minimaal watervolume in het systeem","","","l","20 (6)","20 (6)","20 (6)"]
["","Type (2)","","","","Platenwarmtewisselaar","Platenwarmtewisselaar","Platenwarmtewisselaar"]
["Opgenomen vermogen","Koelen","","Nom.","kW","3.56 (1), 2.17 (2)","4.06 (1), 2.51 (2)","4.58 (1), 3.24 (2)"]
["Sound power level","Koelen","","Nom.","dB(A)","67.0","69.0","69.0"]
["Afmetingen","Unit","","Breedte","mm","1,380","1,380","1,380"]
["","","","Diepte","mm","460","460","460"]
["","","","Hoogte","mm","870","870","870"]
["Capaciteitsregeling","Methode","","","","Variabel (omvormer)","Variabel (omvormer)","Variabel (omvormer)"]
["Ventilator","Luchthoeveelheid","Koelen","Nom.","m³/min","70","85","85"]
["Compressor","Aanloopmethode_","","","","Inverter","Inverter","Inverter"]
["Power supply","Fase","","","","3~","3~","3~"]
["","Frequentie","","","Hz","50","50","50"]
["","Naam","","","","W1","W1","W1"]
["","Spanning","","","V","400","400","400"]
["Opmerkingen","","","","","(1) - Koelen: EW 12℃; LW 7℃; omgevingsomstandigheden: 35°CDB","(1) - Koelen: EW 12℃; LW 7℃; omgevingsomstandigheden: 35°CDB","(1) - Koelen: EW 12℃; LW 7℃; omgevingsomstandigheden: 35°CDB"]
["","","","","","(2) - Koelen: EW 23°C; LW 18°C; omgevingsomstandigheden: 35°CDB","(2) - Koelen: EW 23°C; LW 18°C; omgevingsomstandigheden: 35°CDB","(2) - Koelen: EW 23°C; LW 18°C; omgevingsomstandigheden: 35°CDB"]
["","","","","","(3) - Voorwaarde: Ta DB/NB 7°C/6°C - LWC 35°C (DT = 5°C)","(3) - Voorwaarde: Ta DB/NB 7°C/6°C - LWC 35°C (DT = 5°C)","(3) - Voorwaarde: Ta DB/NB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(4) - Voorwaarde: Ta DB/WB 7 °C / 6 °C - LWC 45 °C (Dt=5 °C)","(4) - Voorwaarde: Ta DB/WB 7 °C / 6 °C - LWC 45 °C (Dt=5 °C)","(4) - Voorwaarde: Ta DB/WB 7 °C / 6 °C - LWC 45 °C (Dt=5 °C)"]
["","","","","","(5) - Overeenkomstig EN14825","(5) - Overeenkomstig EN14825","(5) - Overeenkomstig EN14825"]
["","","","","","(6) - Afhankelijk van de bedrijfsmodus, zie installatiehandleiding","(6) - Afhankelijk van de bedrijfsmodus, zie installatiehandleiding","(6) - Afhankelijk van de bedrijfsmodus, zie installatiehandleiding"]
["","","","","","(7) - Raadpleeg de werkbereik-tekening voor meer informatie","(7) - Raadpleeg de werkbereik-tekening voor meer informatie","(7) - Raadpleeg de werkbereik-tekening voor meer informatie"]