{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":60,"n_cols":9,"rows_kept":60,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EWYA-DW1P-H-"]
[]
[]
[]
[]
["","","","","","EWYA009DAW1P-H-","EWYA011DAW1P-H-","EWYA014DAW1P-H-","EWYA016DAW1P-H-"]
["Geluidsdrukniveau op 1 m","Koelen","","Nom.","dBA","44.0","47.7","50.8","51.0"]
["Hydraulische componenten","Expansievat","","Volume","l","8","8","8","8"]
["Werkingsbereik","Luchtzijdig","Koelen","Min.","°CDB","10","10","10","10"]
["","","","Max.","°CDB","43","43","43","43"]
["","","Verwarmen","Max.","°CDB","25","25","25","25"]
["","","","Min.","°CDB","-25","-25","-25","-25"]
["","Waterkant","Verwarmen","Min.","°CDB","9 (7)","9 (7)","9 (7)","9 (7)"]
["","","","Max.","°CDB","60 (7)","60 (7)","60 (7)","60 (7)"]
["","","Koelen","Max.","°CDB","22","22","22","22"]
["","","","Min.","°CDB","5","5","5","5"]
["Koelmiddelvolume","Per circuit","","","kg","3.80","3.80","3.80","3.80"]
["","Refrigerant charge-=-Per circuit-=-TCO2Eq","","","tCO2eq","2.6","2.6","2.6","2.6"]
["Compressor","Type","","","","Hermetisch gesloten swing-inverter-compressor","Hermetisch gesloten swing-inverter-compressor","Hermetisch gesloten swing-inverter-compressor","Hermetisch gesloten swing-inverter-compressor"]
["","Aanloopmethode_","","","","Invertergestuurd","Invertergestuurd","Invertergestuurd","Invertergestuurd"]
["","Aantal_","","","","1","1","1","1"]
["Luchtgekoelde warmtewisselaar","Type","","","","Uiterst efficiënte lamel en buistype met integrale nakoeler","Uiterst efficiënte lamel en buistype met integrale nakoeler","Uiterst efficiënte lamel en buistype met integrale nakoeler","Uiterst efficiënte lamel en buistype met integrale nakoeler"]
["Gewicht","Unit","","","kg","147","147","147","147"]
["EER","","","","","3.35 (1), 5.34 (2)","3.26 (1), 5.31 (2)","3.16 (1), 5.04 (2)","3.06 (1), 4.74 (2)"]
["Koudemiddel","GWP","","","","675.0","675.0","675.0","675.0"]
["","Type","","","","R-32","R-32","R-32","R-32"]
["","Circuits","","Aantal","","1","1","1","1"]
["","Regeling","","","","Elektronische expansieklep","Elektronische expansieklep","Elektronische expansieklep","Elektronische expansieklep"]
["Ventilatormotor","Snelheid","Koelen","Nom.","rpm","500","550","650","650"]
["","","Verwarmen","Nom.","rpm","400","450","550","650"]
["Totale koelcapaciteit","Nom.","","","kW","9.35 (1), 9.10 (2)","11.6 (1), 11.5 (2)","12.8 (1), 12.7 (2)","14.0 (1), 15.3 (2)"]
["Warmtewisselaar","Watervolume","","","l","2","2","2","2"]
["","Minimaal watervolume in het systeem","","","l","50 (6)","50 (6)","50 (6)","50 (6)"]
["","Type (2)","","","","Platenwarmtewisselaar","Platenwarmtewisselaar","Platenwarmtewisselaar","Platenwarmtewisselaar"]
["Opgenomen vermogen","Koelen","","Nom.","kW","2.79 (1), 1.71 (2)","3.56 (1), 2.17 (2)","4.06 (1), 2.51 (2)","4.58 (1), 3.24 (2)"]
["","Verwarmen","","Nom.","kW","1.91 (3), 2.43 (4)","2.18 (3), 2.68 (4)","2.46 (3), 3.42 (4)","3.53 (3), 4.56 (4)"]
["Geluidsvermogenniveau","Koelen","","Nom.","dBA","65.5","67.0","69.0","69.0"]
["COP","","","","","4.91 (3), 3.71 (4)","4.83 (3), 3.66 (4)","4.87 (3), 3.64 (4)","4.53 (3), 3.51 (4)"]
["Afmetingen","Unit","","Breedte","mm","1,380","1,380","1,380","1,380"]
["","","","Diepte","mm","460","460","460","460"]
["","","","Hoogte","mm","870","870","870","870"]
["Capaciteitsregeling","Methode","","","","Variabel (omvormer)","Variabel (omvormer)","Variabel (omvormer)","Variabel (omvormer)"]
["Verwarming","Wateruitlaat gematigd klimaat 55°C","Algemeen","Seasonal space heating eff. class","","A++","A++","A++","A++"]
["","","","ηs (seizoensefficiëntie ruimteverwarming)","%","135","132","134","132"]
["","","","SCOP","","3.44","3.37","3.42","3.37"]
["Ventilator","Luchthoeveelheid","Verwarmen","Nom.","m³/min","48.0","55.8","70.4","85.0"]
["","","Koelen","Nom.","m³/min","63","70","85","85"]
["Totale verwarmingscapaciteit","Nom.","","","kW","9.37 (3), 9.00 (4)","10.6 (3), 9.82 (4)","12.0 (3), 12.5 (4)","16.0 (3), 16.0 (4)"]
["Compressor","Aanloopmethode_","","","","Inverter","Inverter","Inverter","Inverter"]
["Power supply","Fase","","","","3~","3~","3~","3~"]
["","Frequentie","","","Hz","50","50","50","50"]
["","Naam","","","","W1","W1","W1","W1"]
["","Spanning","","","V","400","400","400","400"]
["Opmerkingen","","","","","(1) - Koelen: EW 12℃; LW 7℃; omgevingsomstandigheden: 35°CDB","(1) - Koelen: EW 12℃; LW 7℃; omgevingsomstandigheden: 35°CDB","(1) - Koelen: EW 12℃; LW 7℃; omgevingsomstandigheden: 35°CDB","(1) - Koelen: EW 12℃; LW 7℃; omgevingsomstandigheden: 35°CDB"]
["","","","","","(2) - Koelen: EW 23°C; LW 18°C; omgevingsomstandigheden: 35°CDB","(2) - Koelen: EW 23°C; LW 18°C; omgevingsomstandigheden: 35°CDB","(2) - Koelen: EW 23°C; LW 18°C; omgevingsomstandigheden: 35°CDB","(2) - Koelen: EW 23°C; LW 18°C; omgevingsomstandigheden: 35°CDB"]
["","","","","","(3) - Voorwaarde: Ta DB/NB 7°C/6°C - LWC 35°C (DT = 5°C)","(3) - Voorwaarde: Ta DB/NB 7°C/6°C - LWC 35°C (DT = 5°C)","(3) - Voorwaarde: Ta DB/NB 7°C/6°C - LWC 35°C (DT = 5°C)","(3) - Voorwaarde: Ta DB/NB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(4) - Voorwaarde: Ta DB/WB 7 °C / 6 °C - LWC 45 °C (Dt=5 °C)","(4) - Voorwaarde: Ta DB/WB 7 °C / 6 °C - LWC 45 °C (Dt=5 °C)","(4) - Voorwaarde: Ta DB/WB 7 °C / 6 °C - LWC 45 °C (Dt=5 °C)","(4) - Voorwaarde: Ta DB/WB 7 °C / 6 °C - LWC 45 °C (Dt=5 °C)"]
["","","","","","(5) - Overeenkomstig EN14825","(5) - Overeenkomstig EN14825","(5) - Overeenkomstig EN14825","(5) - Overeenkomstig EN14825"]
["","","","","","(6) - Afhankelijk van de bedrijfsmodus, zie installatiehandleiding","(6) - Afhankelijk van de bedrijfsmodus, zie installatiehandleiding","(6) - Afhankelijk van de bedrijfsmodus, zie installatiehandleiding","(6) - Afhankelijk van de bedrijfsmodus, zie installatiehandleiding"]
["","","","","","(7) - Raadpleeg de werkbereik-tekening voor meer informatie","(7) - Raadpleeg de werkbereik-tekening voor meer informatie","(7) - Raadpleeg de werkbereik-tekening voor meer informatie","(7) - Raadpleeg de werkbereik-tekening voor meer informatie"]