{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":9,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FAA-B / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FAA71BUV1B / FAA71BUV1B / RZQG100L8Y1B","FAA71BUV1B / FAA71BUV1B / RZQG125L8Y1B","FAA100BUV1B / RZQG100L8Y1B","FAA71BUV1B / RZQG71L8Y1B","FAA100BUV1B / RZQG71L8Y1B"]
["Totale koelcapaciteit","Nom.","","kW","","","","6.80","6.80"]
["Koeling","SEER","","","","","","6.43","6.43"]
["","Jaarlijks energieverbruik","","kWu/a","","","","371","371"]
["","Vermogen","Pdesign","kW","","","","6.80","6.80"]
["","Energieklasse","","","","","","A++","A++"]
["Verwarming (gematigd klimaat)","Vermogen","Pdesign","kW","","","","6.33","6.33"]
["","SCOP/A","","","","","","4.02","4.02"]
["","Energieklasse","","","","","","A+","A+"]
["","Jaarlijks energieverbruik","","kWu/a","","","","2,205","2,205"]
["Nominaal energierendement","EER","","","","","","3.40","3.40"]
["","Jaarlijks energieverbruik","","kWh","","","","1,000"]
["","COP","","","","","","3.70"]
["","Richtlijn Energielabels","Koeling","","","","","A"]
["","","Verwarming","","","","","A"]
["Totale verwarmingscapaciteit","Nom.","","kW","","","","7.50"]
["Bereik van het energierendement","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Opmerkingen","","","","","","","(1) - De nominale koelcapaciteiten zijn gebaseerd op: binnentemperatuur: 27°CDB/19°CNB, buitentemp.: 35°CDB; equivalente koelmiddelleidinglengte: 5m, hoogteverschil: 0 m.","(1) - Zie afzonderlijke afbeelding voor bedrijfsbereik"]
["","","","","","","","(2) - Nominale verwarmingscapaciteiten gebaseerd op: binnentemperatuur: 20°CDB, buitentemperatuur: 7°CDB/6°CWB, equivalente koelmiddelleidinglengte: 5m, hoogteverschil: 0m.","(2) - Voor elektrische gegevens zie afzonderlijke tekening"]
["","","","","","","","(3) - Zie afzonderlijke afbeelding voor bedrijfsbereik"]
["","","","","","","","(4) - Voor elektrische gegevens zie afzonderlijke tekening"]