{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":9,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FAA-B / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FAA71BUV1B / RZQG71L8Y1B","FAA100BUV1B / RZQG71L8Y1B","FAA100BUV1B / RZQG100L8Y1B","FAA71BUV1B / FAA71BUV1B / RZQG100L8Y1B","FAA71BUV1B / FAA71BUV1B / RZQG125L8Y1B"]
["Totale koelcapaciteit","Nom.","","kW","6.80","6.80","9.50","9.50","12.00"]
["Koeling","SEER","","","6.43","6.43","6.11","5.10","5.10"]
["","Jaarlijks energieverbruik","","kWu/a","371","371","545","652","824"]
["","Vermogen","Pdesign","kW","6.80","6.80","9.50","9.50","12.00"]
["","Energieklasse","","","A++","A++","A++","A","A"]
["Verwarming (gematigd klimaat)","Vermogen","Pdesign","kW","6.33","6.33","10.20","11.30","12.71"]
["","SCOP/A","","","4.02","4.02","4.01","3.80","3.80"]
["","Energieklasse","","","A+","A+","A+","A","A"]
["","Jaarlijks energieverbruik","","kWu/a","2,205","2,205","3,562","4,164","4,683"]
["Nominaal energierendement","EER","","","3.40","3.40","3.62","3.75","3.61"]
["","Jaarlijks energieverbruik","","kWu","1,000","","1,312"]
["","COP","","","3.70","","3.61"]
["","Richtlijn Energielabels","Koeling","","A","","A"]
["","","Verwarming","","A","","A"]
["Totale verwarmingscapaciteit","Nom.","","kW","7.50","","10.80"]
["Opmerkingen","","","","(1) - De nominale koelcapaciteiten zijn gebaseerd op: binnentemperatuur: 27°CDB/19°CNB, buitentemp.: 35°CDB; equivalente koelmiddelleidinglengte: 5m, hoogteverschil: 0 m.","(1) - Zie afzonderlijke afbeelding voor bedrijfsbereik","(1) - De nominale koelcapaciteiten zijn gebaseerd op: binnentemperatuur: 27°CDB/19°CNB, buitentemp.: 35°CDB; equivalente koelmiddelleidinglengte: 5m, hoogteverschil: 0 m.","(1) - Zie afzonderlijke afbeelding voor bedrijfsbereik","(1) - Zie afzonderlijke afbeelding voor bedrijfsbereik"]
["","","","","(2) - Nominale verwarmingscapaciteiten gebaseerd op: binnentemperatuur: 20°CDB, buitentemperatuur: 7°CDB/6°CWB, equivalente koelmiddelleidinglengte: 5m, hoogteverschil: 0m.","(2) - Voor elektrische gegevens zie afzonderlijke tekening","(2) - Nominale verwarmingscapaciteiten gebaseerd op: binnentemperatuur: 20°CDB, buitentemperatuur: 7°CDB/6°CWB, equivalente koelmiddelleidinglengte: 5m, hoogteverschil: 0m.","(2) - Voor elektrische gegevens zie afzonderlijke tekening","(2) - Voor elektrische gegevens zie afzonderlijke tekening"]
["","","","","(3) - Zie afzonderlijke afbeelding voor bedrijfsbereik","","(3) - Zie afzonderlijke afbeelding voor bedrijfsbereik"]
["","","","","(4) - Voor elektrische gegevens zie afzonderlijke tekening","","(4) - Voor elektrische gegevens zie afzonderlijke tekening"]