{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":7,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FAA-B"]
[]
[]
[]
[]
["","","","","","FAA71BUV1B","FAA100BUV1B"]
["Behuizing","Kleur","","","","Wit","Wit"]
["","Materiaal","","","","Hars","Hars"]
["Afmetingen","Unit","","Hoogte","mm","290","340"]
["","","","Breedte","mm","1050","1200"]
["","","","Diepte","mm","269","262"]
["Gewicht","Unit","","","kg","14","18"]
["Ventilator-","Luchthoeveelheid","Koelen","Hoog","m³/min","16.2","23"]
["Ventilator","Luchtdebiet","Koeling","Middelhoog","m³/min","13.4","21.1"]
["Ventilator-","Luchthoeveelheid","Koelen","Laag","m³/min","12.1","18.7"]
["","","Verwarmen","Hoog","m³/min","16.9","23"]
["Ventilator","Luchtdebiet","Verwarming","Middelhoog","m³/min","14.2","20.9"]
["Ventilator-","Luchthoeveelheid","Verwarmen","Laag","m³/min","12.7","18.7"]
["Geluidsvermogenniveau","Koelen","","","dB(A)","61","65"]
["","Verwarmen","","","dB(A)","61","65"]
["Geluidsdrukniveau op 1 m","Koelen","","Geluidsdrukniveau op 1 m-=-Koelen-=-Hoog-=-dB(A)","dB(A)","45","49"]
["Geluidsdrukniveau","Koeling","","Middelhoog","dB(A)","42","45"]
["Geluidsdrukniveau op 1 m","Koelen","","Geluidsdrukniveau op 1 m-=-Koelen-=-Laag-=-dB(A)","dB(A)","40","41"]
["","Verwarmen","","Geluidsdrukniveau op 1 m-=-Verwarmen-=-Hoog-=-dB(A)","dB(A)","45","49"]
["Geluidsdrukniveau","Verwarming","","Middelhoog","dB(A)","42","45"]
["Geluidsdrukniveau op 1 m","Verwarmen","","Geluidsdrukniveau op 1 m-=-Verwarmen-=-Laag-=-dB(A)","dB(A)","40","41"]
["Leidingaansluitingen","Vloeistof","","Buitendiameter","mm","9.52","9.52"]
["","Gas","","Buitendiameter","mm","15.9","15.9"]
["","Drainage","","","","VP13 (I.D. 13/O.D. 18)","VP13 (I.D. 13/O.D. 18)"]
["Voeding","Fase","","","","1~","1~"]
["Spanningsvorm","Frequentie","","","Hz","50","50"]
["","Spanning","","","V","220-240","220-240"]
["Standaard-accessoires","Installation plate","","","","1","1"]
["","General safety precautions","","","","1","1"]
["","Wire clamp material","","","","4","4"]
["","Heat insulating tape","","","","1","1"]
["","Installation and operation manual","","","","1","1"]
["","Screw bag","","","","1","1"]
["Opmerkingen","","","","","(1) - De nominale koelcapaciteiten zijn gebaseerd op: binnentemperatuur: 27°CDB/19°CNB, buitentemp.: 35°CDB; equivalente koelmiddelleidinglengte: 5m, hoogteverschil: 0 m."]
["","","","","","(2) - Nominale verwarmingscapaciteiten gebaseerd op: binnentemperatuur: 20°CDB, buitentemperatuur: 7°CDB/6°CWB, equivalente koelmiddelleidinglengte: 5m, hoogteverschil: 0m."]
["Standaard-accessoires","Screw cover","","","","","3"]