{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":9,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FAQ-C9 / RZQG-L9V1"]
[]
[]
[]
[]
["","","","","FAQ100CVEB9 / RZQG71L9V1B","FAQ71CVEB9 / RZQG71L9V1B","FAQ71CVEB9 / FAQ71CVEB9 / RZQG100L9V1B","FAQ100CVEB9 / RZQG100L9V1B","FAQ71CVEB9 / FAQ71CVEB9 / RZQG125L9V1B"]
["Totale koelcapaciteit","Nom.","","kW","","6.8","","9.5"]
["Koeling","SEER","","","6.51","6.43","5.10","6.11","5.10"]
["","Jaarlijks energieverbruik","","kWu/a","366","371","652","545","824"]
["","Vermogen","Pdesign","kW","6.80","6.80","9.50","9.50","12.00"]
["","Energieklasse","","","A++","A++","B","A++","B"]
["Verwarming (gematigd klimaat)","Vermogen","Pdesign","kW","6.33","6.33","11.30","10.20","12.71"]
["","SCOP/A","","","4.02","4.02","3.80","4.01","3.80"]
["","Energieklasse","","","A+","A+","A","A+","A"]
["","Jaarlijks energieverbruik","","kWu/a","2,205","2,205","4,164","3,562","4,683"]
["Nominaal energierendement","Jaarlijks energieverbruik","","kWu","","1,000","","1,315"]
["","EER","","","","3.40","","3.62"]
["","COP","","","","3.70","","3.61"]
["","Richtlijn Energielabels","Koeling","","","A","","A"]
["","","Verwarming","","","A","","A"]
["Totale verwarmingscapaciteit","Nom.","","kW","","7.5","","10.8"]
["Opmerkingen","","","","(1) - EER/COP volgens Eurovent 2012, alleen voor gebruik buiten de EU","","(1) - EER/COP volgens Eurovent 2012, alleen voor gebruik buiten de EU","","(1) - EER/COP volgens Eurovent 2012, alleen voor gebruik buiten de EU"]
["","","","","","(1) - Jaarlijks energieverbruik is conform richtlijn 2002/31/EC inzake energielabels","","(1) - EER/COP volgens Eurovent 2012, alleen voor gebruik buiten de EU"]
["","","","","","(2) - SEER en SCOP zijn conform EN 14825","","(2) - Nominaal rendement: koeling tegen 35°/27° nominale belasting, verwarming tegen 7°/20° nominale belasting"]