{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":6,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBA-A(9) / RXM-A"]
[]
[]
[]
[]
["","","","","FBA50A2VEB9 / RXM50A5V1B","FBA60A2VEB9 / RXM60A5V1B"]
["Totale koelcapaciteit","Nom.","","kW","5.0","5.7"]
["Totale verwarmingscapaciteit","Nom.","","kW","5.5","7"]
["Nominaal rendement","EER","","","3.55","3.48"]
["","COP","","","3.83","3.71"]
["","Jaarlijks energieverbruik","","kWh","704","819"]
["Nominaal energierendement","Richtlijn Energielabels","Koeling","","A","A"]
["","","Verwarming","","A","A"]
["Koeling","Koeling-=-Energieklasse","","","A++","A+"]
["","Vermogen","Pdesign","kW","5.0","5.7"]
["","SEER","","","6.27","5.91"]
["","Jaarlijks energieverbruik","","kWu/a","279","336"]
["Verwarming (gematigd klimaat)","Energieklasse","","","A+","A+"]
["","Vermogen","Pdesign","kW","4.4","4.6"]
["","SCOP/A","","","4.06","4.01"]
["","Pdh-verwarmingsvermogen bij -10 °C","","kW","3.73","3.99"]
["","Jaarlijks energieverbruik","","kWu/a","1,517","1607"]
["Bereik van het energierendement","","","","","A+++ ~ D"]
["Opmerkingen","","","","","(1) - De nominale koelcapaciteiten zijn gebaseerd op: binnentemperatuur: 27°CDB/19°CNB, buitentemp.: 35°CDB; equivalente koelmiddelleidinglengte: 5m, hoogteverschil: 0 m."]
["","","","","","(2) - Nominale verwarmingscapaciteiten gebaseerd op: binnentemperatuur: 20°CDB, buitentemperatuur: 7°CDB/6°CWB, equivalente koelmiddelleidinglengte: 5m, hoogteverschil: 0m."]
["","","","","","(3) - Zie afzonderlijke afbeelding voor bedrijfsbereik"]
["","","","","","(4) - Voor elektrische gegevens zie afzonderlijke tekening"]