{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":18,"n_cols":6,"rows_kept":18,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBQ-C8 / RXS-F"]
[]
[]
[]
[]
["","","","","FBQ60C8VEB / RXS60F3V1B","FBQ60C8VEB / RXS60F4V1B"]
["Totale koelcapaciteit","Nom.","","kW","5.70 (3)","5.70"]
["Nominaal energierendement","Jaarlijks energieverbruik","","kWh","875","875"]
["","EER","","","3.26","3.26"]
["","COP","","","3.41","3.41"]
["","Richtlijn Energielabels","Koeling","","A","A"]
["","","Verwarming","","B","B"]
["Totale verwarmingscapaciteit","Nom.","","kW","7.00 (4)","7.00"]
["Opmerkingen","","","","(1) - Energielabel: schaalverdeling van A (meest efficiënt) tot G (minst efficiënt)","(1) - EER/COP volgens Eurovent 2012, alleen voor gebruik buiten de EU"]
["","","","","(2) - Jaarlijks energieverbruik: op basis van een gemiddelde van 500 bedrijfsuren per jaar bij vollast (nominale omstandigheden)","(2) - Nominaal rendement: koeling tegen 35°/27° nominale belasting, verwarming tegen 7°/20° nominale belasting"]
["","","","","(3) - Koelen: binnentemp. 27°CDB, 19,0°CNB, buitentemp. 35°CDB; equivalente leidinglengte: 5 m; hoogteverschil: 0m"]
["","","","","(4) - Verwarmen: binnentemp. 20°CDB; buitentemp. 7°CDB/6°CWB; equivalente koelmiddelleidinglengte: 5 m; hoogteverschil: 0m"]
["","","","","(5) - Nominaal rendement: koeling tegen 35°/27° nominale belasting, verwarming tegen 7°/20° nominale belasting"]