{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":7,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBQ-C8 / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FBQ35C8VEB / FBQ35C8VEB / RZQG71L8Y1B","FBQ71C8VEB / RZQG71L8Y1B","FBQ140C8VEB / RZQG140L7Y1B"]
["Totale koelcapaciteit","Nom.","","kW","","6.8","13.4"]
["Koeling","SEER","","","5.1","6.11"]
["","Jaarlijks energieverbruik","","kWu/a","467","390"]
["","Vermogen","Pdesign","kW","6.8","6.8"]
["","Energieklasse","","","B","A++"]
["Verwarming (gematigd klimaat)","Vermogen","Pdesign","kW","6","6"]
["","SCOP/A","","","3.8","4.01"]
["","Energieklasse","","","A","A+"]
["","Jaarlijks energieverbruik","","kWu/a","2,211","2,095"]
["Nominaal energierendement","Jaarlijks energieverbruik","","kWu","","970","2,010"]
["","EER","","","","3.50","3.33"]
["","COP","","","","3.65","3.61"]
["","Richtlijn Energielabels","Koeling","","","A"]
["","","Verwarming","","","A"]
["Totale verwarmingscapaciteit","Nom.","","kW","","7.5","15.5"]
["Opmerkingen","","","","(1) - EER/COP volgens Eurovent 2012, alleen voor gebruik buiten de EU"]
["","","","","","(1) - EER/COP volgens Eurovent 2012, alleen voor gebruik buiten de EU","(1) - EER/COP volgens Eurovent 2012, alleen voor gebruik buiten de EU"]
["","","","","","(2) - Nominaal rendement: koeling tegen 35°/27° nominale belasting, verwarming tegen 7°/20° nominale belasting","(2) - Nominaal rendement: koeling tegen 35°/27° nominale belasting, verwarming tegen 7°/20° nominale belasting"]